| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5655: Machine instructions VRSQRTSS VRSQRTPS VRCPSS VRCPPS

Tested procedures
  IiyVRSQRTSS IiyVRSQRTPS IiyVRCPSS IiyVRCPPS

Source & expected listing t5655.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=28, CPU=X64, SIMD=AVX | |t5655 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5EA52CB | VRSQRTSS XMM1,XMM2,XMM3 |00000004:C4E16A52CB | VRSQRTSS XMM1,XMM2,XMM3,PREFIX=VEX3 |00000009:C5EA520E | VRSQRTSS XMM1,XMM2,[RSI] |0000000D:C4E16A520E | VRSQRTSS XMM1,XMM2,[RSI],PREFIX=VEX3 |00000012:C5EA53CB | VRCPSS XMM1,XMM2,XMM3 |00000016:C4E16A53CB | VRCPSS XMM1,XMM2,XMM3,PREFIX=VEX3 |0000001B:C5EA530E | VRCPSS XMM1,XMM2,[RSI] |0000001F:C4E16A530E | VRCPSS XMM1,XMM2,[RSI],PREFIX=VEX3 |00000024:C5F852CA | VRSQRTPS XMM1,XMM2 |00000028:C4E17852CA | VRSQRTPS XMM1,XMM2,PREFIX=VEX3 |0000002D:C5FC52CA | VRSQRTPS YMM1,YMM2 |00000031:C4E17C52CA | VRSQRTPS YMM1,YMM2,PREFIX=VEX3 |00000036:C5F8520E | VRSQRTPS XMM1,[RSI] |0000003A:C4E178520E | VRSQRTPS XMM1,[RSI],PREFIX=VEX3 |0000003F:C5FC520E | VRSQRTPS YMM1,[RSI] |00000043:C4E17C520E | VRSQRTPS YMM1,[RSI],PREFIX=VEX3 |00000048:C5F853CA | VRCPPS XMM1,XMM2 |0000004C:C4E17853CA | VRCPPS XMM1,XMM2,PREFIX=VEX3 |00000051:C5FC53CA | VRCPPS YMM1,YMM2 |00000055:C4E17C53CA | VRCPPS YMM1,YMM2,PREFIX=VEX3 |0000005A:C5F8530E | VRCPPS XMM1,[RSI] |0000005E:C4E178530E | VRCPPS XMM1,[RSI],PREFIX=VEX3 |00000063:C5FC530E | VRCPPS YMM1,[RSI] |00000067:C4E17C530E | VRCPPS YMM1,[RSI],PREFIX=VEX3 | |ENDPROGRAM t5655`

Expected messages t5655.out
  `I0180 Assembling source file "t5655.htm". I0270 Assembling source "t5655". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5655". "t5655.htm"{58} I0510 Assembling program pass 1. "t5655.htm"{58} I0530 Assembling program pass 2 - final. "t5655.htm"{58} I0660 16bit TINY BIN file "t5655.bin" created, size=108. "t5655.htm"{84} I0650 Program "t5655" assembled in 2 passes with errorlevel 0. "t5655.htm"{84} I0750 Source "t5655" (102 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5655.htm.lst" created, size=1635. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲