| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3840: Machine instructions ADDPD ADDSD ANDNPD ANDPD ORPD XORPD DIVPD DIVSD

Tested procedures
  IipGroupSSE IipADDPD IipADDSD IipANDNPD IipANDPD IipORPD IipXORPD IipDIVPD IipDIVSD

Source & expected listing t3840.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE2 | |t3840 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:660F58CF | ADDPD XMM1,XMM7 |0004:660F580C | ADDPD XMM1,[SI] |0008:F20F58CF | ADDSD XMM1,XMM7 |000C:F20F580C | ADDSD XMM1,[SI] |0010:660F55CF | ANDNPD XMM1,XMM7 |0014:660F550C | ANDNPD XMM1,[SI] |0018:660F54CF | ANDPD XMM1,XMM7 |001C:660F540C | ANDPD XMM1,[SI] |0020:660F56CF | ORPD XMM1,XMM7 |0024:660F560C | ORPD XMM1,[SI] |0028:660F57CF | XORPD XMM1,XMM7 |002C:660F570C | XORPD XMM1,[SI] |0030:660F5ECF | DIVPD XMM1,XMM7 |0034:660F5E0C | DIVPD XMM1,[SI] |0038:F20F5ECF | DIVSD XMM1,XMM7 |003C:F20F5E0C | DIVSD XMM1,[SI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660F58CF | ADDPD XMM1,XMM7 |00000004:660F580E | ADDPD XMM1,[ESI] |00000008:F20F58CF | ADDSD XMM1,XMM7 |0000000C:F20F580E | ADDSD XMM1,[ESI] |00000010:660F55CF | ANDNPD XMM1,XMM7 |00000014:660F550E | ANDNPD XMM1,[ESI] |00000018:660F54CF | ANDPD XMM1,XMM7 |0000001C:660F540E | ANDPD XMM1,[ESI] |00000020:660F56CF | ORPD XMM1,XMM7 |00000024:660F560E | ORPD XMM1,[ESI] |00000028:660F57CF | XORPD XMM1,XMM7 |0000002C:660F570E | XORPD XMM1,[ESI] |00000030:660F5ECF | DIVPD XMM1,XMM7 |00000034:660F5E0E | DIVPD XMM1,[ESI] |00000038:F20F5ECF | DIVSD XMM1,XMM7 |0000003C:F20F5E0E | DIVSD XMM1,[ESI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:66450F58CB | ADDPD XMM9,XMM11 |00000005:66440F580E | ADDPD XMM9,[RSI] |0000000A:F20F58CF | ADDSD XMM1,XMM7 |0000000E:67F20F580E | ADDSD XMM1,[ESI] |00000013:660F55CF | ANDNPD XMM1,XMM7 |00000017:660F550C2500000000 | ANDNPD XMM1,[0] |00000020:660F54CF | ANDPD XMM1,XMM7 |00000024:6667460F545C4DF6 | ANDPD XMM11,[2*R9D+EBP-10] |0000002C:66410F56CB | ORPD XMM1,XMM11 |00000031:66410F5609 | ORPD XMM1,[R9] |00000036:66410F57CB | XORPD XMM1,XMM11 |0000003B:66410F5709 | XORPD XMM1,[R9] |00000040:660F5ECF | DIVPD XMM1,XMM7 |00000044:6466670F5E0E | DIVPD XMM1,[FS:ESI] |0000004A:F2440F5ECF | DIVSD XMM9,XMM7 |0000004F:F2440F5E0E | DIVSD XMM9,[RSI] | |ENDPROGRAM t3840`

Expected messages t3840.out
  `I0180 Assembling source file "t3840.htm". I0270 Assembling source "t3840". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3840". "t3840.htm"{73} I0510 Assembling program pass 1. "t3840.htm"{73} I0530 Assembling program pass 2 - final. "t3840.htm"{73} I0660 16bit TINY BIN file "t3840.bin" created, size=212. "t3840.htm"{125} I0650 Program "t3840" assembled in 2 passes with errorlevel 0. "t3840.htm"{125} I0750 Source "t3840" (143 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3840.htm.lst" created, size=2881. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲