| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5646: Machine instructions VSHUFF32X4 VSHUFF64X2 VSHUFI32X4 VSHUFI64X2

Tested procedures
  IizVSHUFF32X4 IizVSHUFF64X2 IizVSHUFI32X4 IizVSHUFI64X2

Source & expected listing t5646.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5646 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F36DAD23CB04 | VSHUFF32X4 YMM1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |00000007:62F36D4D23CB04 | VSHUFF32X4 ZMM1,ZMM2,ZMM3,4,MASK=K5 |0000000E:62F36D2D234D02<504 | VSHUFF32X4 YMM1,YMM2,[RBP+40h],4,MASK=K5 |00000016:62F36D4D234D01<604 | VSHUFF32X4 ZMM1,ZMM2,[RBP+40h],4,MASK=K5 |0000001E:62F36D3D234D10<204 | VSHUFF32X4 YMM1,YMM2,[RBP+40h],4,MASK=K5,BCST=ON |00000026:62F36D5D234D10<204 | VSHUFF32X4 ZMM1,ZMM2,[RBP+40h],4,MASK=K5,BCST=ON |0000002E:62F36DAD43CB04 | VSHUFI32X4 YMM1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |00000035:62F36D4D43CB04 | VSHUFI32X4 ZMM1,ZMM2,ZMM3,4,MASK=K5 |0000003C:62F36D2D434D02<504 | VSHUFI32X4 YMM1,YMM2,[RBP+40h],4,MASK=K5 |00000044:62F36D4D434D01<604 | VSHUFI32X4 ZMM1,ZMM2,[RBP+40h],4,MASK=K5 |0000004C:62F36D3D434D10<204 | VSHUFI32X4 YMM1,YMM2,[RBP+40h],4,MASK=K5,BCST=ON |00000054:62F36D5D434D10<204 | VSHUFI32X4 ZMM1,ZMM2,[RBP+40h],4,MASK=K5,BCST=ON |0000005C:62F3EDAD23CB04 | VSHUFF64X2 YMM1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |00000063:62F3ED4D23CB04 | VSHUFF64X2 ZMM1,ZMM2,ZMM3,4,MASK=K5 |0000006A:62F3ED2D234D02<504 | VSHUFF64X2 YMM1,YMM2,[RBP+40h],4,MASK=K5 |00000072:62F3ED4D234D01<604 | VSHUFF64X2 ZMM1,ZMM2,[RBP+40h],4,MASK=K5 |0000007A:62F3ED3D234D08<304 | VSHUFF64X2 YMM1,YMM2,[RBP+40h],4,MASK=K5,BCST=ON |00000082:62F3ED5D234D08<304 | VSHUFF64X2 ZMM1,ZMM2,[RBP+40h],4,MASK=K5,BCST=ON |0000008A:62F3EDAD43CB04 | VSHUFI64X2 YMM1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |00000091:62F3ED4D43CB04 | VSHUFI64X2 ZMM1,ZMM2,ZMM3,4,MASK=K5 |00000098:62F3ED2D434D02<504 | VSHUFI64X2 YMM1,YMM2,[RBP+40h],4,MASK=K5 |000000A0:62F3ED4D434D01<604 | VSHUFI64X2 ZMM1,ZMM2,[RBP+40h],4,MASK=K5 |000000A8:62F3ED3D434D08<304 | VSHUFI64X2 YMM1,YMM2,[RBP+40h],4,MASK=K5,BCST=ON |000000B0:62F3ED5D434D08<304 | VSHUFI64X2 ZMM1,ZMM2,[RBP+40h],4,MASK=K5,BCST=ON | |ENDPROGRAM t5646`

Expected messages t5646.out
  `I0180 Assembling source file "t5646.htm". I0270 Assembling source "t5646". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5646". "t5646.htm"{58} I0510 Assembling program pass 1. "t5646.htm"{58} I0530 Assembling program pass 2 - final. "t5646.htm"{58} I0660 16bit TINY BIN file "t5646.bin" created, size=184. "t5646.htm"{84} I0650 Program "t5646" assembled in 2 passes with errorlevel 0. "t5646.htm"{84} I0750 Source "t5646" (102 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5646.htm.lst" created, size=2128. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲