| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5606: Machine instructions VPMAXUB VPMAXUW VPMAXUD VPMAXUQ

Tested procedures
  IizVPMAXUB IizVPMAXUW IizVPMAXUD IizVPMAXUQ

Source & expected listing t5606.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5606 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9DECB | VPMAXUB XMM1,XMM2,XMM3 |00000004:C5EDDECB | VPMAXUB YMM1,YMM2,YMM3 |00000008:62F16D0CDECB | VPMAXUB XMM1,XMM2,XMM3,MASK=K4 |0000000E:62F16DACDECB | VPMAXUB YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000014:62F16DCCDECB | VPMAXUB ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000001A:C5E9DE4D40 | VPMAXUB XMM1,XMM2,[RBP+40h] |0000001F:C5EDDE4D40 | VPMAXUB YMM1,YMM2,[RBP+40h] |00000024:62F16D48DE4D01<6 | VPMAXUB ZMM1,ZMM2,[RBP+40h] |0000002B:62F16D0CDE4D04<4 | VPMAXUB XMM1,XMM2,[RBP+40h],MASK=K4 |00000032:62F16DCCDE4D01<6 | VPMAXUB ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000039:C4E2693ECB | VPMAXUW XMM1,XMM2,XMM3 |0000003E:C4E26D3ECB | VPMAXUW YMM1,YMM2,YMM3 |00000043:62F26D0C3ECB | VPMAXUW XMM1,XMM2,XMM3,MASK=K4 |00000049:62F26DAC3ECB | VPMAXUW YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000004F:62F26DCC3ECB | VPMAXUW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000055:C4E2693E4D40 | VPMAXUW XMM1,XMM2,[RBP+40h] |0000005B:C4E26D3E4D40 | VPMAXUW YMM1,YMM2,[RBP+40h] |00000061:62F26D483E4D01<6 | VPMAXUW ZMM1,ZMM2,[RBP+40h] |00000068:62F26D0C3E4D04<4 | VPMAXUW XMM1,XMM2,[RBP+40h],MASK=K4 |0000006F:62F26DAC3E4D02<5 | VPMAXUW YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000076:62F26DCC3E4D01<6 | VPMAXUW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000007D:C4E2693FCB | VPMAXUD XMM1,XMM2,XMM3 |00000082:C4E26D3FCB | VPMAXUD YMM1,YMM2,YMM3 |00000087:62F26D0C3FCB | VPMAXUD XMM1,XMM2,XMM3,MASK=K4 |0000008D:62F26DAC3FCB | VPMAXUD YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000093:62F26DCC3FCB | VPMAXUD ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000099:62F269283FCB | VPMAXUD ZMM1,ZMM2,ZMM3,EH=0,OPER=2 ; MVEX swizzle {badc}. |0000009F:C4E2693F4D40 | VPMAXUD XMM1,XMM2,[RBP+40h] |000000A5:C4E26D3F4D40 | VPMAXUD YMM1,YMM2,[RBP+40h] |000000AB:62F26D483F4D01<6 | VPMAXUD ZMM1,ZMM2,[RBP+40h] |000000B2:62F26D183F4D10<2 | VPMAXUD XMM1,XMM2,[RBP+40h],BCST=ON |000000B9:62F26D383F4D10<2 | VPMAXUD YMM1,YMM2,[RBP+40h],BCST=ON |000000C0:62F26D583F4D10<2 | VPMAXUD ZMM1,ZMM2,[RBP+40h],BCST=ON |000000C7:62F26D0C3F4D04<4 | VPMAXUD XMM1,XMM2,[RBP+40h],MASK=K4 |000000CE:62F26D1C3F4D10<2 | VPMAXUD XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |000000D5:62F26DBC3F4D10<2 | VPMAXUD YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000DC:62F26DCC3F4D01<6 | VPMAXUD ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000E3:62F269083F4D01<6 | VPMAXUD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000EA:62F269183F4D10<2 | VPMAXUD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000F1:62F269283F4D04<4 | VPMAXUD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |000000F8:62F269483F4D04<4 | VPMAXUD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |000000FF:62F2ED083FCB | VPMAXUQ XMM1,XMM2,XMM3 |00000105:62F2EDAC3FCB | VPMAXUQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000010B:62F2EDCC3FCB | VPMAXUQ ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000111:62F2ED083F4D04<4 | VPMAXUQ XMM1,XMM2,[RBP+40h] |00000118:62F2ED283F4D02<5 | VPMAXUQ YMM1,YMM2,[RBP+40h] |0000011F:62F2ED483F4D01<6 | VPMAXUQ ZMM1,ZMM2,[RBP+40h] |00000126:62F2ED183F4D08<3 | VPMAXUQ XMM1,XMM2,[RBP+40h],BCST=ON |0000012D:62F2ED383F4D08<3 | VPMAXUQ YMM1,YMM2,[RBP+40h],BCST=ON |00000134:62F2ED583F4D08<3 | VPMAXUQ ZMM1,ZMM2,[RBP+40h],BCST=ON |0000013B:62F2ED0C3F4D04<4 | VPMAXUQ XMM1,XMM2,[RBP+40h],MASK=K4 |00000142:62F2ED1C3F4D08<3 | VPMAXUQ XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |00000149:62F2EDBC3F4D08<3 | VPMAXUQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000150:62F2EDCC3F4D01<6 | VPMAXUQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5606`

Expected messages t5606.out
  `I0180 Assembling source file "t5606.htm". I0270 Assembling source "t5606". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5606". "t5606.htm"{58} I0510 Assembling program pass 1. "t5606.htm"{58} I0530 Assembling program pass 2 - final. "t5606.htm"{58} I0660 16bit TINY BIN file "t5606.bin" created, size=343. "t5606.htm"{114} I0650 Program "t5606" assembled in 2 passes with errorlevel 0. "t5606.htm"{114} I0750 Source "t5606" (132 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5606.htm.lst" created, size=4046. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲