| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5136: AVX prefix MVEX modifiers.

Description
  Combination of instruction modifiers used with MVEX prefix.

Source & expected listing t5136.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=686, SIMD=AVX512, MVEX=ENABLE, DISPLAYENC=YES | |t5136 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:62F1E90858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |00000006: |; |00000006:62F1E90858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,EH=OFF |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |0000000C: |; |0000000C:62F1E98858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,EH=ON ; Specifying EH in MVEX implies rounding. |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |00000012: |; |00000012:62F1E98858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,ROUND=NEAR |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |00000018: |; |00000018:62F1E99858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,ROUND=DOWN |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=1. |0000001E: |; |0000001E:62F1E9A858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,ROUND=UP |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. |00000024: |; |00000024:62F1E9B858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,ROUND=ZERO |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=3. |0000002A: |; |0000002A:62F1E9A858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,ROUND=UP,EH=ON ; EH is implicitly set when ROUND is specified. |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. |00000030: |; |00000030:62F1E9A858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,ROUND=UP,EH=OFF ; Specifying ROUND in EVEX implies EH=ON. |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. |## W2401 Modifier "EH=OFF" could not be obeyed in this instruction. |00000036: |; |00000036:62F1E90858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=0 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |0000003C: |; |0000003C:62F1E98858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=0,EH=ON ; ROUND is not activated without EH. |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |00000042: |; |00000042:62F1E99858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=1,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=1. |00000048: |; |00000048:62F1E9A858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=2,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. |0000004E: |; |0000004E:62F1E9B858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=3,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=3. |00000054: |; |00000054:62F1E9C858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=4,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=4. |0000005A: |; |0000005A:62F1E9D858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=5,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. |00000060: |; |00000060:62F1E9E858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=6,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=6. |00000066: |; |00000066:62F1E9F858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=7,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=7. |0000006C: |; |0000006C:62F1E9D858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=5,ROUND=ZERO ; Specifying OPER in MVEX overwrites ROUND. |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. |## W2401 Modifier "ROUND=ZERO" could not be obeyed in this instruction. |00000072: |; |00000072:62F1E9D858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=5,ROUND=ZERO,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. |## W2401 Modifier "ROUND=ZERO" could not be obeyed in this instruction. |00000078: |; |00000078:62F1E9D858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=5,ROUND=ZERO,EH=OFF |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. |## W2401 Modifier "EH=OFF,ROUND=ZERO" could not be obeyed in this instruction. |0000007E: |; |0000007E:62F1E9D858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,OPER=5,EH=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. |00000084: |; |00000084:62F1E90858CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K0 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K0,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |0000008A: |; |0000008A:62F1E90958CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K1 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K1,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |00000090: |; |00000090:62F1E90A58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K2 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K2,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |00000096: |; |00000096:62F1E90B58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K3 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K3,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |0000009C: |; |0000009C:62F1E90C58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K4 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |000000A2: |; |000000A2:62F1E90D58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K5 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K5,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |000000A8: |; |000000A8:62F1E90E58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K6 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K6,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |000000AE: |; |000000AE:62F1E90F58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K7 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K7,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |000000B4: |; |000000B4:62F1E90F58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=3+4 ; MASK may be expression evaluated to 0..7. |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K7,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |000000BA: |; |000000BA:62F1E90C58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K4,ZEROING=NO ; ZEROING is not implemented with MVEX. |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |## W2401 Modifier "ZEROING=OFF" could not be obeyed in this instruction. |000000C0: |; |000000C0:62F1E90C58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K4,ZEROING=YES |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. |## W2401 Modifier "ZEROING=ON" could not be obeyed in this instruction. |000000C6: |; |000000C6:62F1E9DC58CB | VADDPD ZMM1,ZMM2,ZMM3,PREFIX=MVEX,MASK=K4,ROUND=DOWN,SAE=ON |# D1080 Emitted size=6,PREFIX=MVEX,EH=ON,MASK=K4,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. |000000CC: |; |000000CC:62F1E908580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. |000000D2: |; |000000D2:62F1E908580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,BCST=OFF ; BCST is not implemented with MVEX, use OPER. |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. |## W2401 Modifier "BCST=OFF" could not be obeyed in this instruction. |000000D8: |; |000000D8:62F1E908580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,BCST=ON ; BCST is not implemented with MVEX, use OPER. |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. |## W2401 Modifier "BCST=ON" could not be obeyed in this instruction. |000000DE: |; |000000DE:62F1E908580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=0 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. |000000E4: |; |000000E4:62F1E918580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=1 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=1,SCALE=SMART,ADDR=ABS. |000000EA: |; |000000EA:62F1E928580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=2 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=2,SCALE=SMART,ADDR=ABS. |000000F0: |; |000000F0:62F1E938580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=3 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=3,SCALE=SMART,ADDR=ABS. |000000F6: |; |000000F6:62F1E948580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=4 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=4,SCALE=SMART,ADDR=ABS. |000000FC: |; |000000FC:62F1E958580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=5 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=5,SCALE=SMART,ADDR=ABS. |00000102: |; |00000102:62F1E968580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=6 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=6,SCALE=SMART,ADDR=ABS. |00000108: |; |00000108:62F1E978580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,OPER=7 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=7,SCALE=SMART,ADDR=ABS. |0000010E: |; |0000010E:62F1E90C580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,MASK=K4 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. |00000114: |; |00000114:62F1E96C580E | VADDPD ZMM1,ZMM2,[ESI],PREFIX=MVEX,MASK=K4,OPER=6 |# D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,DATA=QWORD,DATA=ZWORD,OPER=6,SCALE=SMART,ADDR=ABS. | |ENDPROGRAM t5136`

Expected messages t5136.out
  `I0180 Assembling source file "t5136.htm". I0270 Assembling source "t5136". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5136". "t5136.htm"{47} I0510 Assembling program pass 1. "t5136.htm"{47} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{49} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{52} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{55} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{58} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=1. "t5136.htm"{61} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{64} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=3. "t5136.htm"{67} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{70} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{73} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{77} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{80} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=1. "t5136.htm"{83} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{86} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=3. "t5136.htm"{89} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=4. "t5136.htm"{92} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{95} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=6. "t5136.htm"{98} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=7. "t5136.htm"{101} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{104} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{108} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{112} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{116} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K0,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{119} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K1,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{122} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K2,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{125} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K3,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{128} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{131} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K5,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{134} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K6,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{137} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K7,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{140} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K7,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{143} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{146} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{150} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,MASK=K4,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{154} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{157} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{160} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{164} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{168} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=1,SCALE=SMART,ADDR=ABS. "t5136.htm"{171} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=2,SCALE=SMART,ADDR=ABS. "t5136.htm"{174} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=3,SCALE=SMART,ADDR=ABS. "t5136.htm"{177} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=4,SCALE=SMART,ADDR=ABS. "t5136.htm"{180} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=5,SCALE=SMART,ADDR=ABS. "t5136.htm"{183} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=6,SCALE=SMART,ADDR=ABS. "t5136.htm"{186} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=7,SCALE=SMART,ADDR=ABS. "t5136.htm"{189} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{192} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,DATA=QWORD,DATA=ZWORD,OPER=6,SCALE=SMART,ADDR=ABS. "t5136.htm"{195} I0530 Assembling program pass 2 - final. "t5136.htm"{47} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{49} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{52} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{55} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{58} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=1. "t5136.htm"{61} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{64} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=3. "t5136.htm"{67} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{70} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{73} W2401 Modifier "EH=OFF" could not be obeyed in this instruction. "t5136.htm"{73} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{77} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{80} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=1. "t5136.htm"{83} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=2. "t5136.htm"{86} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=3. "t5136.htm"{89} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=NEAR,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=4. "t5136.htm"{92} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{95} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=UP,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=6. "t5136.htm"{98} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=ZERO,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=7. "t5136.htm"{101} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{104} W2401 Modifier "ROUND=ZERO" could not be obeyed in this instruction. "t5136.htm"{104} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{108} W2401 Modifier "ROUND=ZERO" could not be obeyed in this instruction. "t5136.htm"{108} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{112} W2401 Modifier "EH=OFF,ROUND=ZERO" could not be obeyed in this instruction. "t5136.htm"{112} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{116} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K0,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{119} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K1,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{122} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K2,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{125} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K3,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{128} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{131} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K5,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{134} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K6,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{137} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K7,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{140} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K7,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{143} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{146} W2401 Modifier "ZEROING=OFF" could not be obeyed in this instruction. "t5136.htm"{146} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,SAE=OFF,DATA=QWORD,DATA=ZWORD,OPER=0. "t5136.htm"{150} W2401 Modifier "ZEROING=ON" could not be obeyed in this instruction. "t5136.htm"{150} D1080 Emitted size=6,PREFIX=MVEX,EH=ON,MASK=K4,ROUND=DOWN,SAE=ON,DATA=QWORD,DATA=ZWORD,OPER=5. "t5136.htm"{154} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{157} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{160} W2401 Modifier "BCST=OFF" could not be obeyed in this instruction. "t5136.htm"{160} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{164} W2401 Modifier "BCST=ON" could not be obeyed in this instruction. "t5136.htm"{164} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{168} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=1,SCALE=SMART,ADDR=ABS. "t5136.htm"{171} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=2,SCALE=SMART,ADDR=ABS. "t5136.htm"{174} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=3,SCALE=SMART,ADDR=ABS. "t5136.htm"{177} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=4,SCALE=SMART,ADDR=ABS. "t5136.htm"{180} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=5,SCALE=SMART,ADDR=ABS. "t5136.htm"{183} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=6,SCALE=SMART,ADDR=ABS. "t5136.htm"{186} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,DATA=QWORD,DATA=ZWORD,OPER=7,SCALE=SMART,ADDR=ABS. "t5136.htm"{189} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,DATA=QWORD,DATA=ZWORD,OPER=0,SCALE=SMART,ADDR=ABS. "t5136.htm"{192} D1080 Emitted size=6,PREFIX=MVEX,EH=OFF,MASK=K4,DATA=QWORD,DATA=ZWORD,OPER=6,SCALE=SMART,ADDR=ABS. "t5136.htm"{195} I0660 16bit TINY BIN file "t5136.bin" created, size=282. "t5136.htm"{197} I0650 Program "t5136" assembled in 2 passes with errorlevel 2. "t5136.htm"{197} I0750 Source "t5136" (317 lines) assembled in 2 passes with errorlevel 2. I0860 Listing file "t5136.htm.lst" created, size=10770. I0990 EuroAssembler terminated with errorlevel 2.`

▲Back to the top▲