| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3615: Machine instructions PUNPCKLBW PUNPCKLWD PUNPCKLDQ PACKSSWB PCMPGTB PCMPGTW PCMPGTD PACKUSWB

Tested procedures
  IimGroupSSE2 IimPUNPCKLBW IimPUNPCKLWD IimPUNPCKLDQ IimPACKSSWB IimPCMPGTB IimPCMPGTW IimPCMPGTD IimPACKUSWB

Source & expected listing t3615.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, MMX=ON, SIMD=SSE2 | |t3615 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F60CF | PUNPCKLBW MM1,MM7 |0003:260F6014 | PUNPCKLBW MM2,[ES:SI] |0007:660F60CF | PUNPCKLBW XMM1,XMM7 |000B:660F6056F8 | PUNPCKLBW XMM2,[BP-8] |0010:0F61CF | PUNPCKLWD MM1,MM7 |0013:260F6114 | PUNPCKLWD MM2,[ES:SI] |0017:660F61CF | PUNPCKLWD XMM1,XMM7 |001B:660F6156F8 | PUNPCKLWD XMM2,[BP-8] |0020:0F62CF | PUNPCKLDQ MM1,MM7 |0023:260F6214 | PUNPCKLDQ MM2,[ES:SI] |0027:660F62CF | PUNPCKLDQ XMM1,XMM7 |002B:660F6256F8 | PUNPCKLDQ XMM2,[BP-8] |0030:0F63CF | PACKSSWB MM1,MM7 |0033:260F6314 | PACKSSWB MM2,[ES:SI] |0037:660F63CF | PACKSSWB XMM1,XMM7 |003B:660F6356F8 | PACKSSWB XMM2,[BP-8] |0040:0F64CF | PCMPGTB MM1,MM7 |0043:260F6414 | PCMPGTB MM2,[ES:SI] |0047:660F64CF | PCMPGTB XMM1,XMM7 |004B:660F6456F8 | PCMPGTB XMM2,[BP-8] |0050:0F65CF | PCMPGTW MM1,MM7 |0053:260F6514 | PCMPGTW MM2,[ES:SI] |0057:660F65CF | PCMPGTW XMM1,XMM7 |005B:660F6556F8 | PCMPGTW XMM2,[BP-8] |0060:0F66CF | PCMPGTD MM1,MM7 |0063:260F6614 | PCMPGTD MM2,[ES:SI] |0067:660F66CF | PCMPGTD XMM1,XMM7 |006B:660F6656F8 | PCMPGTD XMM2,[BP-8] |0070:0F67CF | PACKUSWB MM1,MM7 |0073:260F6714 | PACKUSWB MM2,[ES:SI] |0077:660F67CF | PACKUSWB XMM1,XMM7 |007B:660F6756F8 | PACKUSWB XMM2,[BP-8] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F60CF | PUNPCKLBW MM1,MM7 |00000003:0F6016 | PUNPCKLBW MM2,[ESI] |00000006:660F60CF | PUNPCKLBW XMM1,XMM7 |0000000A:66670F6056F8 | PUNPCKLBW XMM2,[BP-8] |00000010:0F61CF | PUNPCKLWD MM1,MM7 |00000013:0F6116 | PUNPCKLWD MM2,[ESI] |00000016:660F61CF | PUNPCKLWD XMM1,XMM7 |0000001A:66670F6156F8 | PUNPCKLWD XMM2,[BP-8] |00000020:0F62CF | PUNPCKLDQ MM1,MM7 |00000023:0F6216 | PUNPCKLDQ MM2,[ESI] |00000026:660F62CF | PUNPCKLDQ XMM1,XMM7 |0000002A:66670F6256F8 | PUNPCKLDQ XMM2,[BP-8] |00000030:0F63CF | PACKSSWB MM1,MM7 |00000033:0F6316 | PACKSSWB MM2,[ESI] |00000036:660F63CF | PACKSSWB XMM1,XMM7 |0000003A:66670F6356F8 | PACKSSWB XMM2,[BP-8] |00000040:0F64CF | PCMPGTB MM1,MM7 |00000043:0F6416 | PCMPGTB MM2,[ESI] |00000046:660F64CF | PCMPGTB XMM1,XMM7 |0000004A:66670F6456F8 | PCMPGTB XMM2,[BP-8] |00000050:0F65CF | PCMPGTW MM1,MM7 |00000053:0F6516 | PCMPGTW MM2,[ESI] |00000056:660F65CF | PCMPGTW XMM1,XMM7 |0000005A:66670F6556F8 | PCMPGTW XMM2,[BP-8] |00000060:0F66CF | PCMPGTD MM1,MM7 |00000063:0F6616 | PCMPGTD MM2,[ESI] |00000066:660F66CF | PCMPGTD XMM1,XMM7 |0000006A:66670F6656F8 | PCMPGTD XMM2,[BP-8] |00000070:0F67CF | PACKUSWB MM1,MM7 |00000073:0F6716 | PACKUSWB MM2,[ESI] |00000076:660F67CF | PACKUSWB XMM1,XMM7 |0000007A:66670F6756F8 | PACKUSWB XMM2,[BP-8] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F60CF | PUNPCKLBW MM1,MM7 |00000003:670F6016 | PUNPCKLBW MM2,[ESI] |00000007:660F60CF | PUNPCKLBW XMM1,XMM7 |0000000B:66410F60542DF8 | PUNPCKLBW XMM2,[R13+RBP-8] |00000012:0F61CF | PUNPCKLWD MM1,MM7 |00000015:670F6116 | PUNPCKLWD MM2,[ESI] |00000019:660F61CF | PUNPCKLWD XMM1,XMM7 |0000001D:66410F61542DF8 | PUNPCKLWD XMM2,[R13+RBP-8] |00000024:0F62CF | PUNPCKLDQ MM1,MM7 |00000027:670F6216 | PUNPCKLDQ MM2,[ESI] |0000002B:660F62CF | PUNPCKLDQ XMM1,XMM7 |0000002F:66410F62542DF8 | PUNPCKLDQ XMM2,[R13+RBP-8] |00000036:0F63CF | PACKSSWB MM1,MM7 |00000039:670F6316 | PACKSSWB MM2,[ESI] |0000003D:660F63CF | PACKSSWB XMM1,XMM7 |00000041:66410F63542DF8 | PACKSSWB XMM2,[R13+RBP-8] |00000048:0F64CF | PCMPGTB MM1,MM7 |0000004B:670F6416 | PCMPGTB MM2,[ESI] |0000004F:660F64CF | PCMPGTB XMM1,XMM7 |00000053:66410F64542DF8 | PCMPGTB XMM2,[R13+RBP-8] |0000005A:0F65CF | PCMPGTW MM1,MM7 |0000005D:670F6516 | PCMPGTW MM2,[ESI] |00000061:660F65CF | PCMPGTW XMM1,XMM7 |00000065:66410F65542DF8 | PCMPGTW XMM2,[R13+RBP-8] |0000006C:0F66CF | PCMPGTD MM1,MM7 |0000006F:670F6616 | PCMPGTD MM2,[ESI] |00000073:660F66CF | PCMPGTD XMM1,XMM7 |00000077:66410F66542DF8 | PCMPGTD XMM2,[R13+RBP-8] |0000007E:0F67CF | PACKUSWB MM1,MM7 |00000081:670F6716 | PACKUSWB MM2,[ESI] |00000085:660F67CF | PACKUSWB XMM1,XMM7 |00000089:66410F67542DF8 | PACKUSWB XMM2,[R13+RBP-8] | |ENDPROGRAM t3615`

Expected messages t3615.out
  `I0180 Assembling source file "t3615.htm". I0270 Assembling source "t3615". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3615". "t3615.htm"{73} I0510 Assembling program pass 1. "t3615.htm"{73} I0530 Assembling program pass 2 - final. "t3615.htm"{73} I0660 16bit TINY BIN file "t3615.bin" created, size=400. "t3615.htm"{173} I0650 Program "t3615" assembled in 2 passes with errorlevel 0. "t3615.htm"{173} I0750 Source "t3615" (191 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3615.htm.lst" created, size=5408. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲