| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5792: Machine instructions VPCMPD VPCMPUD VPCMPQ VPCMPUQ

Tested procedures
  IiyVPCMPD IiyVPCMPUD IiyVPCMPQ IiyVPCMPUQ

Source & expected listing t5792.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5792 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F36D8D1FCB04 | VPCMPD K1,XMM2,XMM3,4,MASK=K5,ZEROING=ON |00000007:62F36DAD1FCB04 | VPCMPD K1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |0000000E:62F36DCD1FCB04 | VPCMPD K1,ZMM2,ZMM3,4,MASK=K5,ZEROING=ON |00000015:62F36D8D1F4D04<404 | VPCMPD K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |0000001D:62F36DAD1F4D02<504 | VPCMPD K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |00000025:62F36DCD1F4D01<604 | VPCMPD K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |0000002D:62F36D9D1F4D10<204 | VPCMPD K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |00000035:62F36DBD1F4D10<204 | VPCMPD K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |0000003D:62F36DDD1F4D10<204 | VPCMPD K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |00000045:62F36D8D1ECB04 | VPCMPUD K1,XMM2,XMM3,4,MASK=K5,ZEROING=ON |0000004C:62F36DAD1ECB04 | VPCMPUD K1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |00000053:62F36DCD1ECB04 | VPCMPUD K1,ZMM2,ZMM3,4,MASK=K5,ZEROING=ON |0000005A:62F36D8D1E4D04<404 | VPCMPUD K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |00000062:62F36DAD1E4D02<504 | VPCMPUD K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |0000006A:62F36DCD1E4D01<604 | VPCMPUD K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |00000072:62F36D9D1E4D10<204 | VPCMPUD K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |0000007A:62F36DBD1E4D10<204 | VPCMPUD K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |00000082:62F36DDD1E4D10<204 | VPCMPUD K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |0000008A:62F3ED8D1FCB04 | VPCMPQ K1,XMM2,XMM3,4,MASK=K5,ZEROING=ON |00000091:62F3EDAD1FCB04 | VPCMPQ K1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |00000098:62F3EDCD1FCB04 | VPCMPQ K1,ZMM2,ZMM3,4,MASK=K5,ZEROING=ON |0000009F:62F3ED8D1F4D04<404 | VPCMPQ K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000A7:62F3EDAD1F4D02<504 | VPCMPQ K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000AF:62F3EDCD1F4D01<604 | VPCMPQ K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000B7:62F3ED9D1F4D08<304 | VPCMPQ K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |000000BF:62F3EDBD1F4D08<304 | VPCMPQ K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |000000C7:62F3EDDD1F4D08<304 | VPCMPQ K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |000000CF:62F3ED8D1ECB04 | VPCMPUQ K1,XMM2,XMM3,4,MASK=K5,ZEROING=ON |000000D6:62F3EDAD1ECB04 | VPCMPUQ K1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |000000DD:62F3EDCD1ECB04 | VPCMPUQ K1,ZMM2,ZMM3,4,MASK=K5,ZEROING=ON |000000E4:62F3ED8D1E4D04<404 | VPCMPUQ K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000EC:62F3EDAD1E4D02<504 | VPCMPUQ K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000F4:62F3EDCD1E4D01<604 | VPCMPUQ K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000FC:62F3ED9D1E4D08<304 | VPCMPUQ K1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |00000104:62F3EDBD1E4D08<304 | VPCMPUQ K1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |0000010C:62F3EDDD1E4D08<304 | VPCMPUQ K1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON | |ENDPROGRAM t5792`

Expected messages t5792.out
  `I0180 Assembling source file "t5792.htm". I0270 Assembling source "t5792". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5792". "t5792.htm"{58} I0510 Assembling program pass 1. "t5792.htm"{58} I0530 Assembling program pass 2 - final. "t5792.htm"{58} I0660 16bit TINY BIN file "t5792.bin" created, size=276. "t5792.htm"{96} I0650 Program "t5792" assembled in 2 passes with errorlevel 0. "t5792.htm"{96} I0750 Source "t5792" (114 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5792.htm.lst" created, size=3163. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲