| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6242: Machine instructions CLEVICT0 CLEVICT1 VPREFETCHNTA VPREFETCHENTA

Tested procedures
  IiyCLEVICT0 IiyCLEVICT1 IiyVPREFETCHNTA IiyVPREFETCHENTA

Source & expected listing t6242.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6242 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5FBAE7D40 | CLEVICT0 [RBP+40h] |00000005:C5FAAE7D40 | CLEVICT1 [RBP+40h] |0000000A:C5F8184540 | VPREFETCHNTA [RBP+40h] |0000000F:C5F8186540 | VPREFETCHENTA [RBP+40h] |00000014:C4E17BAE7D40 | CLEVICT0 [RBP+40h],PREFIX=VEX3 |0000001A:C4E17AAE7D40 | CLEVICT1 [RBP+40h],PREFIX=VEX3 |00000020:C4E178184540 | VPREFETCHNTA [RBP+40h],PREFIX=VEX3 |00000026:C4E178186540 | VPREFETCHENTA [RBP+40h],PREFIX=VEX3 |0000002C:62F17B08AE7D01<6 | CLEVICT0 [RBP+40h],PREFIX=MVEX |00000033:62F17A08AE7D01<6 | CLEVICT1 [RBP+40h],PREFIX=MVEX |0000003A:62F17808184501<6 | VPREFETCHNTA [RBP+40h],PREFIX=MVEX |00000041:62F17808186501<6 | VPREFETCHENTA [RBP+40h],PREFIX=MVEX | |ENDPROGRAM t6242`

Expected messages t6242.out
  `I0180 Assembling source file "t6242.htm". I0270 Assembling source "t6242". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6242". "t6242.htm"{58} I0510 Assembling program pass 1. "t6242.htm"{58} I0530 Assembling program pass 2 - final. "t6242.htm"{58} I0660 16bit TINY BIN file "t6242.bin" created, size=72. "t6242.htm"{72} I0650 Program "t6242" assembled in 2 passes with errorlevel 0. "t6242.htm"{72} I0750 Source "t6242" (90 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6242.htm.lst" created, size=1069. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲