| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3181: Machine instructions CBW, CWDE, CDQE, CWD, CDQ, CQO

Tested procedures
  IigCBW IigCWDE IigCDQE IigCWD IigCDQ IigCQO

Source & expected listing t3181.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=24, CPU=X64 | |t3181 PROGRAM FORMAT=BIN,MODEL=TINY,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:98 | CBW |0001:6698 | CWDE |0003:99 | CWD |0004:6699 | CDQ |0006: | |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:6698 | CBW |00000002:98 | CWDE |00000003:6699 | CWD |00000005:99 | CDQ |00000006: | |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:6698 | CBW |00000002:98 | CWDE |00000003:4898 | CDQE |00000005:6699 | CWD |00000007:99 | CDQ |00000008:4899 | CQO |0000000A: | | | ENDPROGRAM t3181`

Expected messages t3181.out
  `I0180 Assembling source file "t3181.htm". I0270 Assembling source "t3181". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3181". "t3181.htm"{64} I0510 Assembling program pass 1. "t3181.htm"{64} I0530 Assembling program pass 2 - final. "t3181.htm"{64} I0660 16bit TINY BIN file "t3181.bin" created, size=42. "t3181.htm"{85} I0650 Program "t3181" assembled in 2 passes with errorlevel 0. "t3181.htm"{85} I0750 Source "t3181" (103 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3181.htm.lst" created, size=902. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲