| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t2570: Pseudoinstruction %COMMENT%

Source & expected listing t2570.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=16 | |t2570 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[BIN] |[BIN] SEGMENT WIDTH=16,PURPOSE=DATA |0000:EE | DB 0xEE ; Emitted data. | | %COMMENT | | DB 0xCC ; Commented-out data (not emitted). | | %ENDCOMMENT |0001:EE | DB 0xEE ; Emitted data. | | %COMMENT | | DB 0xCC ; Commented-out data (not emitted). | | %COMMENT | | DB 0xDD ; Double-commented-out data (not emitted). | | %ENDCOMMENT | | DB 0xCC ; Commented-out data (not emitted). | | %ENDCOMMENT |0002:EE | DB 0xEE ; Emitted data. | | ENDPROGRAM t2570`

Expected messages t2570.out
  `I0180 Assembling source file "t2570.htm". I0270 Assembling source "t2570". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t2570". "t2570.htm"{42} I0510 Assembling program pass 1. "t2570.htm"{42} I0530 Assembling program pass 2 - final. "t2570.htm"{42} I0660 16bit TINY BIN file "t2570.bin" created, size=3. "t2570.htm"{57} I0650 Program "t2570" assembled in 2 passes with errorlevel 0. "t2570.htm"{57} I0750 Source "t2570" (80 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t2570.htm.lst" created, size=871. I0990 EuroAssembler terminated with errorlevel 0.`

Expected output file t2570. bin

      0000: EE EE EE                                         ¤¤¤

▲Back to the top▲