| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3133: Machine instructions NOP NOP1 NOP2 NOP3 NOP4 NOP5 NOP6 NOP7 NOP8 NOP9 in 64bit mode

Tested procedures
  IisNOP IisNOP1 IisNOP2 IisNOP3 IisNOP4 IisNOP5 IisNOP6 IisNOP7 IisNOP8 IisNOP9

Source & expected listing t3133.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64 | |t3133 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:90 | NOP |00000001:6690 | OTOGGLE NOP |00000003:0F1F00 | NOP [RAX],DATA=DWORD |00000006:0F1F4000 | NOP [RAX],DATA=DWORD,DISP=BYTE |0000000A:0F1F442000 | NOP [RAX+0*RAX],DATA=DWORD,SCALE=VERBATIM,DISP=BYTE |0000000F:660F1F442000 | NOP [RAX+0*RAX],DATA=WORD,SCALE=VERBATIM,DISP=BYTE |00000015:0F1F8000000000 | NOP [RAX],DATA=DWORD,DISP=DWORD |0000001C:0F1F842000000000 | NOP [RAX+0*RAX],DATA=DWORD,SCALE=VERBATIM,DISP=DWORD |00000024:660F1F842000000000 | NOP [RAX+0*RAX],DATA=WORD,SCALE=VERBATIM,DISP=DWORD |0000002D:90 | NOP1 |0000002E:6690 | NOP2 |00000030:0F1F00 | NOP3 |00000033:0F1F4000 | NOP4 |00000037:0F1F442000 | NOP5 |0000003C:660F1F442000 | NOP6 |00000042:0F1F8000000000 | NOP7 |00000049:0F1F842000000000 | NOP8 |00000051:660F1F842000000000 | NOP9 | |ENDPROGRAM t3133`

Expected messages t3133.out
  `I0180 Assembling source file "t3133.htm". I0270 Assembling source "t3133". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3133". "t3133.htm"{76} I0510 Assembling program pass 1. "t3133.htm"{76} I0530 Assembling program pass 2 - final. "t3133.htm"{76} I0660 16bit TINY BIN file "t3133.bin" created, size=90. "t3133.htm"{96} I0650 Program "t3133" assembled in 2 passes with errorlevel 0. "t3133.htm"{96} I0750 Source "t3133" (114 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3133.htm.lst" created, size=1212. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲