| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5664: Machine instructions VEXP2PS VEXP2PD

Tested procedures
  IiyVEXP2PS IiyVEXP2PD

Source & expected listing t5664.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5664 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27DDBC8CA | VEXP2PS ZMM1,ZMM2,MASK=K3,ZEROING=ON,SAE=ON |00000006:62F27DCBC84D01<6 | VEXP2PS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |0000000D:62F27DDBC84D10<2 | VEXP2PS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |00000014:62F2FD5BC8CA | VEXP2PD ZMM1,ZMM2,MASK=K3,SAE=ON |0000001A:62F2FDCBC84D01<6 | VEXP2PD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000021:62F2FDDBC84D08<3 | VEXP2PD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON | |ENDPROGRAM t5664`

Expected messages t5664.out
  `I0180 Assembling source file "t5664.htm". I0270 Assembling source "t5664". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5664". "t5664.htm"{52} I0510 Assembling program pass 1. "t5664.htm"{52} I0530 Assembling program pass 2 - final. "t5664.htm"{52} I0660 16bit TINY BIN file "t5664.bin" created, size=40. "t5664.htm"{60} I0650 Program "t5664" assembled in 2 passes with errorlevel 0. "t5664.htm"{60} I0750 Source "t5664" (78 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5664.htm.lst" created, size=753. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲