| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3685: Machine instructions MOVNTSS MOVNTSD

Tested procedures
  IipMOVNTSS IipMOVNTSD

Source & expected listing t3685.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=34, CPU=X64, AMD=ON, SIMD=SSE4 | |t3685 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:F30F2B14 | MOVNTSS [SI],XMM2 |0004:67F30F2B16 | MOVNTSS [ESI],XMM2 |0009:F30F2B16[0800] | MOVNTSS [MemDword],XMM2 |000F:F20F2B14 | MOVNTSD [SI],XMM2 |0013:67F20F2B16 | MOVNTSD [ESI],XMM2 |0018:F20F2B16[0000] | MOVNTSD [MemQword],XMM2 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:67F30F2B14 | MOVNTSS [SI],XMM2 |00000005:F30F2B16 | MOVNTSS [ESI],XMM2 |00000009:F30F2B15[08000000] | MOVNTSS [MemDword],XMM2 |00000011:67F20F2B14 | MOVNTSD [SI],XMM2 |00000016:F20F2B16 | MOVNTSD [ESI],XMM2 |0000001A:F20F2B15[00000000] | MOVNTSD [MemQword],XMM2 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0000000000000000 |MemQword DQ 0 |00000008:00000000 |MemDword DD 0 |0000000C:F30F2B16 | MOVNTSS [RSI],XMM2 |00000010:67F30F2B16 | MOVNTSS [ESI],XMM2 |00000015:F3440F2B26 | MOVNTSS [RSI],XMM12 |0000001A:F30F2B15E6FFFFFF | MOVNTSS [MemDword],XMM2 |00000022:F20F2B16 | MOVNTSD [RSI],XMM2 |00000026:67F20F2B16 | MOVNTSD [ESI],XMM2 |0000002B:F2440F2B25CCFFFFFF | MOVNTSD [MemQword],XMM12 |00000034:F2440F2B2425[00000000] | MOVNTSD [MemQword],XMM12,ADDR=ABS | | ENDPROGRAM t3685`

Expected messages t3685.out
  `I0180 Assembling source file "t3685.htm". I0270 Assembling source "t3685". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3685". "t3685.htm"{52} I0510 Assembling program pass 1. "t3685.htm"{52} I0510 Assembling program pass 2. "t3685.htm"{52} I0530 Assembling program pass 3 - final. "t3685.htm"{52} I0660 16bit TINY BIN file "t3685.bin" created, size=142. "t3685.htm"{78} I0650 Program "t3685" assembled in 3 passes with errorlevel 0. "t3685.htm"{78} I0750 Source "t3685" (97 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3685.htm.lst" created, size=1727. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲