| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3860: Machine instructions ADDSUBPD HADDPD HADDPS HSUBPD HSUBPS MOVDDUP MOVSHDUP MOVSLDUP

Tested procedures
  IipGroupSSE IipADDSUBPD IipHADDPD IipHADDPS IipHSUBPD IipHSUBPS IipMOVDDUP IipMOVSHDUP IipMOVSLDUP

Source & expected listing t3860.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE3 | |t3860 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:660FD0CF | ADDSUBPD XMM1,XMM7 |0004:660FD00C | ADDSUBPD XMM1,[SI] |0008:660F7CCF | HADDPD XMM1,XMM7 |000C:660F7C0C | HADDPD XMM1,[SI] |0010:F20F7CCF | HADDPS XMM1,XMM7 |0014:F20F7C0C | HADDPS XMM1,[SI] |0018:660F7DCF | HSUBPD XMM1,XMM7 |001C:660F7D0C | HSUBPD XMM1,[SI] |0020:F20F7DCF | HSUBPS XMM1,XMM7 |0024:F20F7D0C | HSUBPS XMM1,[SI] |0028:F20F12CF | MOVDDUP XMM1,XMM7 |002C:F20F120C | MOVDDUP XMM1,[SI] |0030:F30F16CF | MOVSHDUP XMM1,XMM7 |0034:F30F160C | MOVSHDUP XMM1,[SI] |0038:F30F12CF | MOVSLDUP XMM1,XMM7 |003C:F30F120C | MOVSLDUP XMM1,[SI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660FD0CF | ADDSUBPD XMM1,XMM7 |00000004:660FD00E | ADDSUBPD XMM1,[ESI] |00000008:660F7CCF | HADDPD XMM1,XMM7 |0000000C:660F7C0E | HADDPD XMM1,[ESI] |00000010:F20F7CCF | HADDPS XMM1,XMM7 |00000014:F20F7C0E | HADDPS XMM1,[ESI] |00000018:660F7DCF | HSUBPD XMM1,XMM7 |0000001C:660F7D0E | HSUBPD XMM1,[ESI] |00000020:F20F7DCF | HSUBPS XMM1,XMM7 |00000024:F20F7D0E | HSUBPS XMM1,[ESI] |00000028:F20F12CF | MOVDDUP XMM1,XMM7 |0000002C:F20F120E | MOVDDUP XMM1,[ESI] |00000030:F30F16CF | MOVSHDUP XMM1,XMM7 |00000034:F30F160E | MOVSHDUP XMM1,[ESI] |00000038:F30F12CF | MOVSLDUP XMM1,XMM7 |0000003C:F30F120E | MOVSLDUP XMM1,[ESI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:66450FD0CB | ADDSUBPD XMM9,XMM11 |00000005:66440FD00E | ADDSUBPD XMM9,[RSI] |0000000A:660F7CCF | HADDPD XMM1,XMM7 |0000000E:66670F7C0E | HADDPD XMM1,[ESI] |00000013:F20F7CCF | HADDPS XMM1,XMM7 |00000017:F20F7C0C2500000000 | HADDPS XMM1,[0] |00000020:660F7DCF | HSUBPD XMM1,XMM7 |00000024:6667460F7D5C4DF6 | HSUBPD XMM11,[2*R9D+EBP-10] |0000002C:F2410F7DCB | HSUBPS XMM1,XMM11 |00000031:F2410F7D09 | HSUBPS XMM1,[R9] |00000036:F2410F12CB | MOVDDUP XMM1,XMM11 |0000003B:F2410F1209 | MOVDDUP XMM1,[R9] |00000040:F30F16CF | MOVSHDUP XMM1,XMM7 |00000044:6467F30F160E | MOVSHDUP XMM1,[FS:ESI] |0000004A:F3440F12CF | MOVSLDUP XMM9,XMM7 |0000004F:F3440F120E | MOVSLDUP XMM9,[RSI] | |ENDPROGRAM t3860`

Expected messages t3860.out
  `I0180 Assembling source file "t3860.htm". I0270 Assembling source "t3860". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3860". "t3860.htm"{73} I0510 Assembling program pass 1. "t3860.htm"{73} I0530 Assembling program pass 2 - final. "t3860.htm"{73} I0660 16bit TINY BIN file "t3860.bin" created, size=212. "t3860.htm"{125} I0650 Program "t3860" assembled in 2 passes with errorlevel 0. "t3860.htm"{125} I0750 Source "t3860" (143 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3860.htm.lst" created, size=2971. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲