| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6126: Machine instructions VGMAXABSPS VGMINPS VGMAXPS

Tested procedures
  IiyVGMAXABSPS IiyVGMINPS IiyVGMAXPS

Source & expected listing t6126.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6126 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2690C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000006:62F2691C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; {cdab}. |0000000C:62F2692C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; {badc}. |00000012:62F2693C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=3 ; {dacb}. |00000018:62F2694C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; {aaaa}. |0000001E:62F2695C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=5 ; {bbbb}. |00000024:62F2696C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=6 ; {cccc}. |0000002A:62F2697C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=7 ; {dddd}. |00000030:62F2690C514D01<6 | VGMAXABSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000037:62F2691C514D10<2 | VGMAXABSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=1 ; {1to16}. |0000003E:62F2692C514D04<4 | VGMAXABSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. |00000045:62F2693C514D02<5 | VGMAXABSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=3 ; {float16}. |0000004C:62F2694C514D04<4 | VGMAXABSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=4 ; {uint8}. |00000053:62F2696C514D02<5 | VGMAXABSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=6 ; {uint16}. |0000005A:62F2697C514D02<5 | VGMAXABSPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=7 ; {sint16}. |00000061:62F269CC51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,SAE=ON,EH=1 |00000067:62F2694C51CB | VGMAXABSPS ZMM1,ZMM2,ZMM3,MASK=K4,SAE=ON |0000006D:62F2690C52CB | VGMINPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000073:62F2690C524D01<6 | VGMINPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |0000007A:62F2690C53CB | VGMAXPS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 ; {dcba}. |00000080:62F2690C534D01<6 | VGMAXPS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. | |ENDPROGRAM t6126`

Expected messages t6126.out
  `I0180 Assembling source file "t6126.htm". I0270 Assembling source "t6126". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6126". "t6126.htm"{55} I0510 Assembling program pass 1. "t6126.htm"{55} I0530 Assembling program pass 2 - final. "t6126.htm"{55} I0660 16bit TINY BIN file "t6126.bin" created, size=135. "t6126.htm"{78} I0650 Program "t6126" assembled in 2 passes with errorlevel 0. "t6126.htm"{78} I0750 Source "t6126" (96 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6126.htm.lst" created, size=2128. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲