| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5422: Machine instructions VFMSUBADD132PS VFMSUBADD213PS VFMSUBADD231PS VFMSUBADD132PD VFMSUBADD213PD VFMSUBADD231PD

Tested procedures
  IibVFMSUBADD132PS IibVFMSUBADD213PS IibVFMSUBADD231PS IibVFMSUBADD132PD IibVFMSUBADD213PD IibVFMSUBADD231PD

Source & expected listing t5422.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,SIMD=AVX512,FMA=ON,EVEX=ON | |t5422 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E26997CB | VFMSUBADD132PS XMM1,XMM2,XMM3 |00000005:C4E269974D40 | VFMSUBADD132PS XMM1,XMM2,[RBP+40h] |0000000B:62F26D0C974D04<4 | VFMSUBADD132PS XMM1,XMM2,[RBP+40h],MASK=K4 |00000012:62F26D18974D10<2 | VFMSUBADD132PS XMM1,XMM2,[RBP+40h],BCST=ON |00000019:C4E26D97CB | VFMSUBADD132PS YMM1,YMM2,YMM3 |0000001E:C4E26D974D40 | VFMSUBADD132PS YMM1,YMM2,[RBP+40h] |00000024:62F26DAC974D02<5 | VFMSUBADD132PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000002B:62F26D38974D10<2 | VFMSUBADD132PS YMM1,YMM2,[RBP+40h],BCST=ON |00000032:62F26D4897CB | VFMSUBADD132PS ZMM1,ZMM2,ZMM3 |00000038:62F26D7897CB | VFMSUBADD132PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |0000003E:62F26D48974D01<6 | VFMSUBADD132PS ZMM1,ZMM2,[RBP+40h] |00000045:62F26DCC974D01<6 | VFMSUBADD132PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000004C:62F26D58974D10<2 | VFMSUBADD132PS ZMM1,ZMM2,[RBP+40h],BCST=ON |00000053:C4E269A7CB | VFMSUBADD213PS XMM1,XMM2,XMM3 |00000058:C4E269A74D40 | VFMSUBADD213PS XMM1,XMM2,[RBP+40h] |0000005E:62F26D0CA74D04<4 | VFMSUBADD213PS XMM1,XMM2,[RBP+40h],MASK=K4 |00000065:62F26D18A74D10<2 | VFMSUBADD213PS XMM1,XMM2,[RBP+40h],BCST=ON |0000006C:C4E26DA7CB | VFMSUBADD213PS YMM1,YMM2,YMM3 |00000071:C4E26DA74D40 | VFMSUBADD213PS YMM1,YMM2,[RBP+40h] |00000077:62F26DACA74D02<5 | VFMSUBADD213PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000007E:62F26D38A74D10<2 | VFMSUBADD213PS YMM1,YMM2,[RBP+40h],BCST=ON |00000085:62F26D48A7CB | VFMSUBADD213PS ZMM1,ZMM2,ZMM3 |0000008B:62F26D78A7CB | VFMSUBADD213PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |00000091:62F26D48A74D01<6 | VFMSUBADD213PS ZMM1,ZMM2,[RBP+40h] |00000098:62F26DCCA74D01<6 | VFMSUBADD213PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000009F:62F26D58A74D10<2 | VFMSUBADD213PS ZMM1,ZMM2,[RBP+40h],BCST=ON |000000A6:C4E269B7CB | VFMSUBADD231PS XMM1,XMM2,XMM3 |000000AB:C4E269B74D40 | VFMSUBADD231PS XMM1,XMM2,[RBP+40h] |000000B1:62F26D0CB74D04<4 | VFMSUBADD231PS XMM1,XMM2,[RBP+40h],MASK=K4 |000000B8:62F26D18B74D10<2 | VFMSUBADD231PS XMM1,XMM2,[RBP+40h],BCST=ON |000000BF:C4E26DB7CB | VFMSUBADD231PS YMM1,YMM2,YMM3 |000000C4:C4E26DB74D40 | VFMSUBADD231PS YMM1,YMM2,[RBP+40h] |000000CA:62F26DACB74D02<5 | VFMSUBADD231PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000D1:62F26D38B74D10<2 | VFMSUBADD231PS YMM1,YMM2,[RBP+40h],BCST=ON |000000D8:62F26D48B7CB | VFMSUBADD231PS ZMM1,ZMM2,ZMM3 |000000DE:62F26D78B7CB | VFMSUBADD231PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |000000E4:62F26D48B74D01<6 | VFMSUBADD231PS ZMM1,ZMM2,[RBP+40h] |000000EB:62F26DCCB74D01<6 | VFMSUBADD231PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000F2:62F26D58B74D10<2 | VFMSUBADD231PS ZMM1,ZMM2,[RBP+40h],BCST=ON |000000F9:C4E2E997CB | VFMSUBADD132PD XMM1,XMM2,XMM3 |000000FE:C4E2E9974D40 | VFMSUBADD132PD XMM1,XMM2,[RBP+40h] |00000104:62F2ED0C974D04<4 | VFMSUBADD132PD XMM1,XMM2,[RBP+40h],MASK=K4 |0000010B:62F2ED18974D08<3 | VFMSUBADD132PD XMM1,XMM2,[RBP+40h],BCST=ON |00000112:C4E2ED97CB | VFMSUBADD132PD YMM1,YMM2,YMM3 |00000117:C4E2ED974D40 | VFMSUBADD132PD YMM1,YMM2,[RBP+40h] |0000011D:62F2EDAC974D02<5 | VFMSUBADD132PD YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000124:62F2ED38974D08<3 | VFMSUBADD132PD YMM1,YMM2,[RBP+40h],BCST=ON |0000012B:62F2ED4897CB | VFMSUBADD132PD ZMM1,ZMM2,ZMM3 |00000131:62F2ED7897CB | VFMSUBADD132PD ZMM1,ZMM2,ZMM3,ROUND=ZERO |00000137:62F2ED48974D01<6 | VFMSUBADD132PD ZMM1,ZMM2,[RBP+40h] |0000013E:62F2EDCC974D01<6 | VFMSUBADD132PD ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000145:62F2ED58974D08<3 | VFMSUBADD132PD ZMM1,ZMM2,[RBP+40h],BCST=ON |0000014C:C4E2E9A7CB | VFMSUBADD213PD XMM1,XMM2,XMM3 |00000151:C4E2E9A74D40 | VFMSUBADD213PD XMM1,XMM2,[RBP+40h] |00000157:62F2ED0CA74D04<4 | VFMSUBADD213PD XMM1,XMM2,[RBP+40h],MASK=K4 |0000015E:62F2ED18A74D08<3 | VFMSUBADD213PD XMM1,XMM2,[RBP+40h],BCST=ON |00000165:C4E2EDA7CB | VFMSUBADD213PD YMM1,YMM2,YMM3 |0000016A:C4E2EDA74D40 | VFMSUBADD213PD YMM1,YMM2,[RBP+40h] |00000170:62F2EDACA74D02<5 | VFMSUBADD213PD YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000177:62F2ED38A74D08<3 | VFMSUBADD213PD YMM1,YMM2,[RBP+40h],BCST=ON |0000017E:62F2ED48A7CB | VFMSUBADD213PD ZMM1,ZMM2,ZMM3 |00000184:62F2ED78A7CB | VFMSUBADD213PD ZMM1,ZMM2,ZMM3,ROUND=ZERO |0000018A:62F2ED48A74D01<6 | VFMSUBADD213PD ZMM1,ZMM2,[RBP+40h] |00000191:62F2EDCCA74D01<6 | VFMSUBADD213PD ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000198:62F2ED58A74D08<3 | VFMSUBADD213PD ZMM1,ZMM2,[RBP+40h],BCST=ON |0000019F:C4E2E9B7CB | VFMSUBADD231PD XMM1,XMM2,XMM3 |000001A4:C4E2E9B74D40 | VFMSUBADD231PD XMM1,XMM2,[RBP+40h] |000001AA:62F2ED0CB74D04<4 | VFMSUBADD231PD XMM1,XMM2,[RBP+40h],MASK=K4 |000001B1:62F2ED18B74D08<3 | VFMSUBADD231PD XMM1,XMM2,[RBP+40h],BCST=ON |000001B8:C4E2EDB7CB | VFMSUBADD231PD YMM1,YMM2,YMM3 |000001BD:C4E2EDB74D40 | VFMSUBADD231PD YMM1,YMM2,[RBP+40h] |000001C3:62F2EDACB74D02<5 | VFMSUBADD231PD YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000001CA:62F2ED38B74D08<3 | VFMSUBADD231PD YMM1,YMM2,[RBP+40h],BCST=ON |000001D1:62F2ED48B7CB | VFMSUBADD231PD ZMM1,ZMM2,ZMM3 |000001D7:62F2ED78B7CB | VFMSUBADD231PD ZMM1,ZMM2,ZMM3,ROUND=ZERO |000001DD:62F2ED48B74D01<6 | VFMSUBADD231PD ZMM1,ZMM2,[RBP+40h] |000001E4:62F2EDCCB74D01<6 | VFMSUBADD231PD ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000001EB:62F2ED58B74D08<3 | VFMSUBADD231PD ZMM1,ZMM2,[RBP+40h],BCST=ON | |ENDPROGRAM t5422`

Expected messages t5422.out
  `I0180 Assembling source file "t5422.htm". I0270 Assembling source "t5422". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5422". "t5422.htm"{64} I0510 Assembling program pass 1. "t5422.htm"{64} I0530 Assembling program pass 2 - final. "t5422.htm"{64} I0660 16bit TINY BIN file "t5422.bin" created, size=498. "t5422.htm"{144} I0650 Program "t5422" assembled in 2 passes with errorlevel 0. "t5422.htm"{144} I0750 Source "t5422" (162 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5422.htm.lst" created, size=6240. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲