| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5732: Machine instructions VPOR VPORD VPORQ

Tested procedures
  IiyVPORD IiyVPORQ IiyVPOR

Source & expected listing t5732.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5732 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9EBCB | VPOR XMM1,XMM2,XMM3 |00000004:C5EDEBCB | VPOR YMM1,YMM2,YMM3 |00000008:C5E9EB4D40 | VPOR XMM1,XMM2,[RBP+40h] |0000000D:C5EDEB4D40 | VPOR YMM1,YMM2,[RBP+40h] |00000012:62F16D08EBCB | VPORD XMM1,XMM2,XMM3 |00000018:62F16D28EBCB | VPORD YMM1,YMM2,YMM3 |0000001E:62F16D8CEBCB | VPORD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000024:62F16DACEBCB | VPORD YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000002A:62F16DCCEBCB | VPORD ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000030:62F1692CEBCB | VPORD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; MVEX {badc}. |00000036:62F1694CEBCB | VPORD ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; MVEX {aaaa}. |0000003C:62F16D08EB4D04<4 | VPORD XMM1,XMM2,[RBP+40h],BCST=OFF |00000043:62F16D28EB4D02<5 | VPORD YMM1,YMM2,[RBP+40h],BCST=OFF |0000004A:62F16D48EB4D01<6 | VPORD ZMM1,ZMM2,[RBP+40h],BCST=OFF |00000051:62F16D18EB4D10<2 | VPORD XMM1,XMM2,[RBP+40h],BCST=ON |00000058:62F16D38EB4D10<2 | VPORD YMM1,YMM2,[RBP+40h],BCST=ON |0000005F:62F16D58EB4D10<2 | VPORD ZMM1,ZMM2,[RBP+40h],BCST=ON |00000066:62F16908EB4D01<6 | VPORD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |0000006D:62F16918EB4D10<2 | VPORD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |00000074:62F16928EB4D04<4 | VPORD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |0000007B:62F1ED8CEBCB | VPORQ XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000081:62F1EDACEBCB | VPORQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000087:62F1EDCCEBCB | VPORQ ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000008D:62F1E92CEBCB | VPORQ ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; MVEX {badc}. |00000093:62F1E94CEBCB | VPORQ ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; MVEX {aaaa}. |00000099:62F1ED8CEB4D04<4 | VPORQ XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000A0:62F1EDACEB4D02<5 | VPORQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000A7:62F1EDCCEB4D01<6 | VPORQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000AE:62F1ED9CEB4D08<3 | VPORQ XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000B5:62F1EDBCEB4D08<3 | VPORQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000BC:62F1EDDCEB4D08<3 | VPORQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000C3:62F1E908EB4D01<6 | VPORQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000CA:62F1E918EB4D08<3 | VPORQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000D1:62F1E928EB4D02<5 | VPORQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. | |ENDPROGRAM t5732`

Expected messages t5732.out
  `I0180 Assembling source file "t5732.htm". I0270 Assembling source "t5732". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5732". "t5732.htm"{55} I0510 Assembling program pass 1. "t5732.htm"{55} I0530 Assembling program pass 2 - final. "t5732.htm"{55} I0660 16bit TINY BIN file "t5732.bin" created, size=216. "t5732.htm"{91} I0650 Program "t5732" assembled in 2 passes with errorlevel 0. "t5732.htm"{91} I0750 Source "t5732" (109 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5732.htm.lst" created, size=2859. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲