| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5250: Machine instructions VALIGND VALIGNQ

Tested procedures
  IizVALIGND IizVALIGNQ

Source & expected listing t5250.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=34, DUMPALL=OFF, CPU=X64, SIMD=AVX512, MVEX=ON, EVEX=ON | |t5250 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F36D0803CB04 | VALIGND XMM1,XMM2,XMM3,4 |00000007:62F36D0D03CB04 | VALIGND XMM1,XMM2,XMM3,4,MASK=K5 |0000000E:62F36D08034D04<404 | VALIGND XMM1,XMM2,[RBP+40h],4 |00000016:62F36D18034D10<204 | VALIGND XMM1,XMM2,[RBP+40h],4,BCST=ON |0000001E:62F36D1D034D10<204 | VALIGND XMM1,XMM2,[RBP+40h],4,BCST=ON,MASK=K5 |00000026:62F36D2803CB04 | VALIGND YMM1,YMM2,YMM3,4 |0000002D:62F36D2D03CB04 | VALIGND YMM1,YMM2,YMM3,4,MASK=K5 |00000034:62F36D28034D02<504 | VALIGND YMM1,YMM2,[RBP+40h],4 |0000003C:62F36D38034D10<204 | VALIGND YMM1,YMM2,[RBP+40h],4,BCST=ON |00000044:62F36D4803CB04 | VALIGND ZMM1,ZMM2,ZMM3,4 |0000004B:62F36D48034D01<604 | VALIGND ZMM1,ZMM2,[RBP+40h],4 |00000053:62F36D58034D10<204 | VALIGND ZMM1,ZMM2,[RBP+40h],4,BCST=ON |0000005B:62F36D5D034D10<204 | VALIGND ZMM1,ZMM2,[RBP+40h],4,BCST=ON,MASK=K5 |00000063:62F3690803CB04 | VALIGND ZMM1,ZMM2,ZMM3,4,PREFIX=MVEX |0000006A:62F36908034D02<504 | VALIGND ZMM1,ZMM2,[RBP+40h],4,PREFIX=MVEX |00000072:62F3690D034D02<504 | VALIGND ZMM1,ZMM2,[RBP+40h],4,PREFIX=MVEX,MASK=K5 |0000007A:62F3698803CB04 | VALIGND ZMM1,ZMM2,ZMM3,4,EH=ON |00000081:62F3698D03CB04 | VALIGND ZMM1,ZMM2,ZMM3,4,EH=ON,MASK=K5 |00000088: | |00000088:62F3ED0803CB04 | VALIGNQ XMM1,XMM2,XMM3,4 |0000008F:62F3ED0D03CB04 | VALIGNQ XMM1,XMM2,XMM3,4,MASK=K5 |00000096:62F3ED08034D04<404 | VALIGNQ XMM1,XMM2,[RBP+40h],4 |0000009E:62F3ED18034D08<304 | VALIGNQ XMM1,XMM2,[RBP+40h],4,BCST=ON |000000A6:62F3ED1D034D08<304 | VALIGNQ XMM1,XMM2,[RBP+40h],4,BCST=ON,MASK=K5 |000000AE:62F3ED2803CB04 | VALIGNQ YMM1,YMM2,YMM3,4 |000000B5:62F3ED2D03CB04 | VALIGNQ YMM1,YMM2,YMM3,4,MASK=K5 |000000BC:62F3ED28034D02<504 | VALIGNQ YMM1,YMM2,[RBP+40h],4 |000000C4:62F3ED38034D08<304 | VALIGNQ YMM1,YMM2,[RBP+40h],4,BCST=ON |000000CC:62F3ED4803CB04 | VALIGNQ ZMM1,ZMM2,ZMM3,4 |000000D3:62F3ED48034D01<604 | VALIGNQ ZMM1,ZMM2,[RBP+40h],4 |000000DB:62F3ED58034D08<304 | VALIGNQ ZMM1,ZMM2,[RBP+40h],4,BCST=ON |000000E3:62F3ED5D034D08<304 | VALIGNQ ZMM1,ZMM2,[RBP+40h],4,BCST=ON,MASK=K5 | |ENDPROGRAM t5250`

Expected messages t5250.out
  `I0180 Assembling source file "t5250.htm". I0270 Assembling source "t5250". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5250". "t5250.htm"{52} I0510 Assembling program pass 1. "t5250.htm"{52} I0530 Assembling program pass 2 - final. "t5250.htm"{52} I0660 16bit TINY BIN file "t5250.bin" created, size=235. "t5250.htm"{86} I0650 Program "t5250" assembled in 2 passes with errorlevel 0. "t5250.htm"{86} I0750 Source "t5250" (104 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5250.htm.lst" created, size=2569. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲