| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5468: Machine instructions VPMASKMOVD VPMASKMOVQ

Tested procedures
  IiyVPMASKMOVD IiyVPMASKMOVQ

Source & expected listing t5468.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,SIMD=AVX2 | |t5668 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:C4E2698C0E | VPMASKMOVD XMM1,XMM2,[ESI] |00000005:C4E26D8C0E | VPMASKMOVD YMM1,YMM2,[ESI] |0000000A:C4E2698E1F | VPMASKMOVD [EDI],XMM2,XMM3 |0000000F:C4E26D8E1F | VPMASKMOVD [EDI],YMM2,YMM3 |00000014:C4E2E98C0E | VPMASKMOVQ XMM1,XMM2,[ESI] |00000019:C4E2ED8C0E | VPMASKMOVQ YMM1,YMM2,[ESI] |0000001E:C4E2E98E1F | VPMASKMOVQ [EDI],XMM2,XMM3 |00000023:C4E2ED8E1F | VPMASKMOVQ [EDI],YMM2,YMM3 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:67C4E2698C0E | VPMASKMOVD XMM1,XMM2,[ESI] |00000006:67C4E26D8C0E | VPMASKMOVD YMM1,YMM2,[ESI] |0000000C:67C4E2698E1F | VPMASKMOVD [EDI],XMM2,XMM3 |00000012:67C4E26D8E1F | VPMASKMOVD [EDI],YMM2,YMM3 |00000018:67C4E2E98C0E | VPMASKMOVQ XMM1,XMM2,[ESI] |0000001E:67C4E2ED8C0E | VPMASKMOVQ YMM1,YMM2,[ESI] |00000024:67C4E2E98E1F | VPMASKMOVQ [EDI],XMM2,XMM3 |0000002A:67C4E2ED8E1F | VPMASKMOVQ [EDI],YMM2,YMM3 |00000030:C4E2698C0E | VPMASKMOVD XMM1,XMM2,[RSI] |00000035:C4E26D8C0E | VPMASKMOVD YMM1,YMM2,[RSI] |0000003A:C4E2698E1F | VPMASKMOVD [RDI],XMM2,XMM3 |0000003F:C4E26D8E1F | VPMASKMOVD [RDI],YMM2,YMM3 |00000044:C4E2E98C0E | VPMASKMOVQ XMM1,XMM2,[RSI] |00000049:C4E2ED8C0E | VPMASKMOVQ YMM1,YMM2,[RSI] |0000004E:C4E2E98E1F | VPMASKMOVQ [RDI],XMM2,XMM3 |00000053:C4E2ED8E1F | VPMASKMOVQ [RDI],YMM2,YMM3 |00000058:67C482ED8E5C7500 | VPMASKMOVQ [R13D+2*R14D],YMM2,YMM3 | |ENDPROGRAM t5668`

Expected messages t5468.out
  `I0180 Assembling source file "t5468.htm". I0270 Assembling source "t5468". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5668". "t5468.htm"{52} I0510 Assembling program pass 1. "t5468.htm"{52} I0530 Assembling program pass 2 - final. "t5468.htm"{52} I0660 16bit TINY BIN file "t5668.bin" created, size=144. "t5468.htm"{80} I0650 Program "t5668" assembled in 2 passes with errorlevel 0. "t5468.htm"{80} I0750 Source "t5468" (98 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5468.htm.lst" created, size=1784. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲