| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5684: Machine instructions VPAVGB VPAVGW

Tested procedures
  IiyVPAVGB IiyVPAVGW

Source & expected listing t5684.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5684 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9E0CB | VPAVGB XMM1,XMM2,XMM3 |00000004:C5EDE0CB | VPAVGB YMM1,YMM2,YMM3 |00000008:C4E169E0CB | VPAVGB XMM1,XMM2,XMM3,PREFIX=VEX3 |0000000D:C4E16DE0CB | VPAVGB YMM1,YMM2,YMM3,PREFIX=VEX3 |00000012:62F16D8CE0CB | VPAVGB XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000018:62F16DACE0CB | VPAVGB YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000001E:62F16DCCE0CB | VPAVGB ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000024:C5E9E04D40 | VPAVGB XMM1,XMM2,[RBP+40h] |00000029:C5EDE04D40 | VPAVGB YMM1,YMM2,[RBP+40h] |0000002E:C4E169E04D40 | VPAVGB XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000034:C4E16DE04D40 | VPAVGB YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |0000003A:62F16D8CE04D04<4 | VPAVGB XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000041:62F16DACE04D02<5 | VPAVGB YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000048:62F16DCCE04D01<6 | VPAVGB ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000004F:C5E9E3CB | VPAVGW XMM1,XMM2,XMM3 |00000053:C5EDE3CB | VPAVGW YMM1,YMM2,YMM3 |00000057:C4E169E3CB | VPAVGW XMM1,XMM2,XMM3,PREFIX=VEX3 |0000005C:C4E16DE3CB | VPAVGW YMM1,YMM2,YMM3,PREFIX=VEX3 |00000061:62F16D8CE3CB | VPAVGW XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000067:62F16DACE3CB | VPAVGW YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000006D:62F16DCCE3CB | VPAVGW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000073:C5E9E34D40 | VPAVGW XMM1,XMM2,[RBP+40h] |00000078:C5EDE34D40 | VPAVGW YMM1,YMM2,[RBP+40h] |0000007D:C4E169E34D40 | VPAVGW XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000083:C4E16DE34D40 | VPAVGW YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |00000089:62F16D8CE34D04<4 | VPAVGW XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000090:62F16DACE34D02<5 | VPAVGW YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000097:62F16DCCE34D01<6 | VPAVGW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5684`

Expected messages t5684.out
  `I0180 Assembling source file "t5684.htm". I0270 Assembling source "t5684". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5684". "t5684.htm"{52} I0510 Assembling program pass 1. "t5684.htm"{52} I0530 Assembling program pass 2 - final. "t5684.htm"{52} I0660 16bit TINY BIN file "t5684.bin" created, size=158. "t5684.htm"{82} I0650 Program "t5684" assembled in 2 passes with errorlevel 0. "t5684.htm"{82} I0750 Source "t5684" (100 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5684.htm.lst" created, size=2206. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲