| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4101: Machine instructions ENCODEKEY128, ENCODEKEY256, AESENC128KL, AESDEC128KL, AESENC256KL, AESDEC256KL, AESENCWIDE128KL, AESDECWIDE128KL, AESENCWIDE256KL, AESDECWIDE256KL

Source & expected listing t4101.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE1, AES=ENABLED | |t4101 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:F30F38FAC3 | ENCODEKEY128 EAX,EBX |0005:F30F38FBC3 | ENCODEKEY256 EAX,EBX |000A:F30F38DC0C | AESENC128KL XMM1,[SI] |000F:F30F38DD15 | AESDEC128KL XMM2,[DI] |0014:F30F38DE1F | AESENC256KL XMM3,[BX] |0019:F30F38DF6600 | AESDEC256KL XMM4,[BP] |001F:F30F38D804 | AESENCWIDE128KL [SI] |0024:F30F38D80D | AESDECWIDE128KL [DI] |0029:F30F38D817 | AESENCWIDE256KL [BX] |002E:F30F38D85E00 | AESDECWIDE256KL [BP] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:F30F38FAC3 | ENCODEKEY128 EAX,EBX |00000005:F30F38FBC3 | ENCODEKEY256 EAX,EBX |0000000A:F30F38DC0E | AESENC128KL XMM1,[ESI] |0000000F:F30F38DD17 | AESDEC128KL XMM2,[EDI] |00000014:F30F38DE1B | AESENC256KL XMM3,[EBX] |00000019:F30F38DF6500 | AESDEC256KL XMM4,[EBP] |0000001F:F30F38D806 | AESENCWIDE128KL [ESI] |00000024:F30F38D80F | AESDECWIDE128KL [EDI] |00000029:F30F38D813 | AESENCWIDE256KL [EBX] |0000002E:F30F38D85D00 | AESDECWIDE256KL [EBP] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:F30F38FAC3 | ENCODEKEY128 EAX,EBX |00000005:F30F38FBC3 | ENCODEKEY256 EAX,EBX |0000000A:F30F38DC0E | AESENC128KL XMM1,[RSI] |0000000F:F30F38DD17 | AESDEC128KL XMM2,[RDI] |00000014:F30F38DE1B | AESENC256KL XMM3,[RBX] |00000019:F30F38DF6500 | AESDEC256KL XMM4,[RBP] |0000001F:F30F38D806 | AESENCWIDE128KL [RSI] |00000024:F30F38D80F | AESDECWIDE128KL [RDI] |00000029:F30F38D813 | AESENCWIDE256KL [RBX] |0000002E:F30F38D85D00 | AESDECWIDE256KL [RBP] | |ENDPROGRAM t4101`

Expected messages t4101.out
  `I0180 Assembling source file "t4101.htm". I0270 Assembling source "t4101". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4101". "t4101.htm"{42} I0510 Assembling program pass 1. "t4101.htm"{42} I0530 Assembling program pass 2 - final. "t4101.htm"{42} I0660 16bit TINY BIN file "t4101.bin" created, size=180. "t4101.htm"{76} I0650 Program "t4101" assembled in 2 passes with errorlevel 0. "t4101.htm"{76} I0750 Source "t4101" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4101.htm.lst" created, size=2140. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲