| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6134: Machine instructions VEXP223PS VLOG2PS VRCP23PS VRSQRT23PS

Tested procedures
  IiyVEXP223PS IiyVLOG2PS IiyVRCP23PS IiyVRSQRT23PS

Source & expected listing t6134.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6134 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2790BC8CA | VEXP223PS ZMM1,ZMM2,MASK=K3,EH=0,OPER=0 ; No swizzle. |00000006:62F279CCC8CA | VEXP223PS ZMM1,ZMM2,MASK=K4,EH=1,SAE=ON |0000000C:62F279CCC8CA | VEXP223PS ZMM1,ZMM2,MASK=K4,EH=1,OPER=4 |00000012:62F2790CC84D01<6 | VEXP223PS ZMM1,[RBP+40h],MASK=K4,OPER=0 ; No broadcast. |00000019:62F2790BC9CA | VLOG2PS ZMM1,ZMM2,MASK=K3,EH=0,OPER=0 ; No swizzle. |0000001F:62F279CCC9CA | VLOG2PS ZMM1,ZMM2,MASK=K4,EH=1,SAE=ON |00000025:62F279CCC9CA | VLOG2PS ZMM1,ZMM2,MASK=K4,EH=1,OPER=4 |0000002B:62F2790CC94D01<6 | VLOG2PS ZMM1,[RBP+40h],MASK=K4,OPER=0 ; No broadcast. |00000032:62F2790BCACA | VRCP23PS ZMM1,ZMM2,MASK=K3,EH=0,OPER=0 ; No swizzle. |00000038:62F279CCCACA | VRCP23PS ZMM1,ZMM2,MASK=K4,EH=1,SAE=ON |0000003E:62F279CCCACA | VRCP23PS ZMM1,ZMM2,MASK=K4,EH=1,OPER=4 |00000044:62F2790CCA4D01<6 | VRCP23PS ZMM1,[RBP+40h],MASK=K4,OPER=0 ; No broadcast. |0000004B:62F2790BCBCA | VRSQRT23PS ZMM1,ZMM2,MASK=K3,EH=0,OPER=0 ; No swizzle. |00000051:62F279CCCBCA | VRSQRT23PS ZMM1,ZMM2,MASK=K4,EH=1,SAE=ON |00000057:62F279CCCBCA | VRSQRT23PS ZMM1,ZMM2,MASK=K4,EH=1,OPER=4 |0000005D:62F2790CCB4D01<6 | VRSQRT23PS ZMM1,[RBP+40h],MASK=K4,OPER=0 ; No broadcast. | |ENDPROGRAM t6134`

Expected messages t6134.out
  `I0180 Assembling source file "t6134.htm". I0270 Assembling source "t6134". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6134". "t6134.htm"{58} I0510 Assembling program pass 1. "t6134.htm"{58} I0530 Assembling program pass 2 - final. "t6134.htm"{58} I0660 16bit TINY BIN file "t6134.bin" created, size=100. "t6134.htm"{76} I0650 Program "t6134" assembled in 2 passes with errorlevel 0. "t6134.htm"{76} I0750 Source "t6134" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6134.htm.lst" created, size=1565. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲