| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5240: Machine instructions VBROADCASTSS VBROADCASTSD VBROADCASTF128

Tested procedures
  IizVBROADCASTSS IizVBROADCASTSD IizVBROADCASTF128

Source & expected listing t5240.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,CPU=X64,SIMD=AVX512,MVEX=ON, EVEX=ON | |t5240 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E27D1A4D40 | VBROADCASTF128 YMM1,[RBP+40h] |00000006:C4E279184D40 | VBROADCASTSS XMM1,[RBP+40h] |0000000C:C4E27D184D40 | VBROADCASTSS YMM1,[RBP+40h] |00000012:62F27D0A184D10<2 | VBROADCASTSS XMM1,[RBP+40h],MASK=K2 |00000019:62F27D0818CA | VBROADCASTSS XMM1,XMM2 |0000001F:62F27D2A184D10<2 | VBROADCASTSS YMM1,[RBP+40h],MASK=K2 |00000026:62F27D2818CA | VBROADCASTSS YMM1,XMM2 |0000002C:62F27D4818CA | VBROADCASTSS ZMM1,XMM2 |00000032:62F27DCB184D10<2 | VBROADCASTSS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000039:62F2798B184D10<2 | VBROADCASTSS ZMM1,[RBP+40h],MASK=K3,EH=ON |00000040:62F27938184D20<1 | VBROADCASTSS ZMM1,[RBP+40h],PREFIX=MVEX, \ |00000047: | OPER=3 ; Convert from float16 to float32. |00000047:62F27948184D40 | VBROADCASTSS ZMM1,[RBP+40h],PREFIX=MVEX, \ |0000004E: | OPER=4 ; Convert from uint8 to float32. |0000004E:C4E27D194D40 | VBROADCASTSD YMM1,[RBP+40h] |00000054:62F2FD2A194D08<3 | VBROADCASTSD YMM1,[RBP+40h],MASK=K2 |0000005B:62F2FD2819CA | VBROADCASTSD YMM1,XMM2 |00000061:62F2FD4819CA | VBROADCASTSD ZMM1,XMM2 |00000067:62F2FDCA194D08<3 | VBROADCASTSD ZMM1,[RBP+40h],MASK=K2,ZEROING=ON |0000006E:62F2F98A194D08<3 | VBROADCASTSD ZMM1,[RBP+40h],MASK=K2,EH=ON,OPER=0 | |ENDPROGRAM t5240`

Expected messages t5240.out
  `I0180 Assembling source file "t5240.htm". I0270 Assembling source "t5240". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5240". "t5240.htm"{55} I0510 Assembling program pass 1. "t5240.htm"{55} I0530 Assembling program pass 2 - final. "t5240.htm"{55} I0660 16bit TINY BIN file "t5240.bin" created, size=117. "t5240.htm"{77} I0650 Program "t5240" assembled in 2 passes with errorlevel 0. "t5240.htm"{77} I0750 Source "t5240" (95 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5240.htm.lst" created, size=1762. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲