| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5401: Machine instructions VFMADD312SS VFMADD123SS VFMADD321SS VFMSUB312SS VFMSUB123SS VFMSUB321SS

Tested procedures
  IibVFMADD312SS IibVFMADD123SS IibVFMADD321SS IibVFMSUB312SS IibVFMSUB123SS IibVFMSUB321SS

Source & expected listing t5401.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,SIMD=AVX512,FMA=ON,EVEX=ON | |t5401 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E26999CB | VFMADD312SS XMM1,XMM2,XMM3 |00000005:62F26D5899CB | VFMADD312SS XMM1,XMM2,XMM3,ROUND=UP |0000000B:62F26D8C99CB | VFMADD312SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000011:62F26D8C994D10<2 | VFMADD312SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000018:C4E269A9CB | VFMADD123SS XMM1,XMM2,XMM3 |0000001D:62F26D58A9CB | VFMADD123SS XMM1,XMM2,XMM3,ROUND=UP |00000023:62F26D8CA9CB | VFMADD123SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000029:62F26D8CA94D10<2 | VFMADD123SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000030:C4E269B9CB | VFMADD321SS XMM1,XMM2,XMM3 |00000035:62F26D58B9CB | VFMADD321SS XMM1,XMM2,XMM3,ROUND=UP |0000003B:62F26D8CB9CB | VFMADD321SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000041:62F26D8CB94D10<2 | VFMADD321SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000048:C4E2699BCB | VFMSUB312SS XMM1,XMM2,XMM3 |0000004D:62F26D589BCB | VFMSUB312SS XMM1,XMM2,XMM3,ROUND=UP |00000053:62F26D8C9BCB | VFMSUB312SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000059:62F26D8C9B4D10<2 | VFMSUB312SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000060:C4E269ABCB | VFMSUB123SS XMM1,XMM2,XMM3 |00000065:62F26D58ABCB | VFMSUB123SS XMM1,XMM2,XMM3,ROUND=UP |0000006B:62F26D8CABCB | VFMSUB123SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000071:62F26D8CAB4D10<2 | VFMSUB123SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000078:C4E269BBCB | VFMSUB321SS XMM1,XMM2,XMM3 |0000007D:62F26D58BBCB | VFMSUB321SS XMM1,XMM2,XMM3,ROUND=UP |00000083:62F26D8CBBCB | VFMSUB321SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000089:62F26D8CBB4D10<2 | VFMSUB321SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5401`

Expected messages t5401.out
  `I0180 Assembling source file "t5401.htm". I0270 Assembling source "t5401". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5401". "t5401.htm"{64} I0510 Assembling program pass 1. "t5401.htm"{64} I0530 Assembling program pass 2 - final. "t5401.htm"{64} I0660 16bit TINY BIN file "t5401.bin" created, size=144. "t5401.htm"{90} I0650 Program "t5401" assembled in 2 passes with errorlevel 0. "t5401.htm"{90} I0750 Source "t5401" (108 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5401.htm.lst" created, size=2160. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲