| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5410: Machine instructions VFMADD132PS VFMADD213PS VFMADD231PS VFMSUB132PS VFMSUB213PS VFMSUB231PS VFMADD233PS

Tested procedures
  IibVFMADD132PS IibVFMADD213PS IibVFMADD231PS IibVFMSUB132PS IibVFMSUB213PS IibVFMSUB231PS IizVFMADD233PS

Source & expected listing t5410.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,SIMD=AVX512,FMA=ON,EVEX=ON, MVEX=ON | |t5410 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E26998CB | VFMADD132PS XMM1,XMM2,XMM3 |00000005:C4E269984D40 | VFMADD132PS XMM1,XMM2,[RBP+40h] |0000000B:62F26D0C984D04<4 | VFMADD132PS XMM1,XMM2,[RBP+40h],MASK=K4 |00000012:62F26D18984D10<2 | VFMADD132PS XMM1,XMM2,[RBP+40h],BCST=ON |00000019:C4E26D98CB | VFMADD132PS YMM1,YMM2,YMM3 |0000001E:C4E26D984D40 | VFMADD132PS YMM1,YMM2,[RBP+40h] |00000024:62F26DAC984D02<5 | VFMADD132PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000002B:62F26D38984D10<2 | VFMADD132PS YMM1,YMM2,[RBP+40h],BCST=ON |00000032:62F26D4898CB | VFMADD132PS ZMM1,ZMM2,ZMM3 |00000038:62F26D7898CB | VFMADD132PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |0000003E:62F2691C98CB | VFMADD132PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; Swap inner pairs {cdab}. |00000044:62F2699C98CB | VFMADD132PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; Round down. |0000004A:62F26D48984D01<6 | VFMADD132PS ZMM1,ZMM2,[RBP+40h] |00000051:62F26DCC984D01<6 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000058:62F26D58984D10<2 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],BCST=ON |0000005F:62F26908984D01<6 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |00000066:62F26918984D10<2 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |0000006D:62F26928984D04<4 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000074:62F26938984D02<5 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=3 ; {float16}. |0000007B:62F26948984D04<4 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |00000082:62F26968984D02<5 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=6 ; {uint16}. |00000089:62F26978984D02<5 | VFMADD132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=7 ; {sint16}. |00000090:C4E269A8CB | VFMADD213PS XMM1,XMM2,XMM3 |00000095:C4E269A84D40 | VFMADD213PS XMM1,XMM2,[RBP+40h] |0000009B:62F26D0CA84D04<4 | VFMADD213PS XMM1,XMM2,[RBP+40h],MASK=K4 |000000A2:62F26D18A84D10<2 | VFMADD213PS XMM1,XMM2,[RBP+40h],BCST=ON |000000A9:C4E26DA8CB | VFMADD213PS YMM1,YMM2,YMM3 |000000AE:C4E26DA84D40 | VFMADD213PS YMM1,YMM2,[RBP+40h] |000000B4:62F26DACA84D02<5 | VFMADD213PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000BB:62F26D38A84D10<2 | VFMADD213PS YMM1,YMM2,[RBP+40h],BCST=ON |000000C2:62F26D48A8CB | VFMADD213PS ZMM1,ZMM2,ZMM3 |000000C8:62F26D78A8CB | VFMADD213PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |000000CE:62F2691CA8CB | VFMADD213PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; Swap inner pairs {cdab}. |000000D4:62F2699CA8CB | VFMADD213PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; Round down. |000000DA:62F26D48A84D01<6 | VFMADD213PS ZMM1,ZMM2,[RBP+40h] |000000E1:62F26DCCA84D01<6 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000E8:62F26D58A84D10<2 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],BCST=ON |000000EF:62F26908A84D01<6 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000F6:62F26918A84D10<2 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000FD:62F26928A84D04<4 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000104:62F26938A84D02<5 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=3 ; {float16}. |0000010B:62F26948A84D04<4 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |00000112:62F26968A84D02<5 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=6 ; {uint16}. |00000119:62F26978A84D02<5 | VFMADD213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=7 ; {sint16}. |00000120:C4E269B8CB | VFMADD231PS XMM1,XMM2,XMM3 |00000125:C4E269B84D40 | VFMADD231PS XMM1,XMM2,[RBP+40h] |0000012B:62F26D0CB84D04<4 | VFMADD231PS XMM1,XMM2,[RBP+40h],MASK=K4 |00000132:62F26D18B84D10<2 | VFMADD231PS XMM1,XMM2,[RBP+40h],BCST=ON |00000139:C4E26DB8CB | VFMADD231PS YMM1,YMM2,YMM3 |0000013E:C4E26DB84D40 | VFMADD231PS YMM1,YMM2,[RBP+40h] |00000144:62F26DACB84D02<5 | VFMADD231PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000014B:62F26D38B84D10<2 | VFMADD231PS YMM1,YMM2,[RBP+40h],BCST=ON |00000152:62F26D48B8CB | VFMADD231PS ZMM1,ZMM2,ZMM3 |00000158:62F26D78B8CB | VFMADD231PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |0000015E:62F2691CB8CB | VFMADD231PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; Swap inner pairs {cdab}. |00000164:62F2699CB8CB | VFMADD231PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; Round down. |0000016A:62F26D48B84D01<6 | VFMADD231PS ZMM1,ZMM2,[RBP+40h] |00000171:62F26DCCB84D01<6 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000178:62F26D58B84D10<2 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],BCST=ON |0000017F:62F26908B84D01<6 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |00000186:62F26918B84D10<2 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |0000018D:62F26928B84D04<4 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000194:62F26938B84D02<5 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=3 ; {float16}. |0000019B:62F26948B84D04<4 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |000001A2:62F26968B84D02<5 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=6 ; {uint16}. |000001A9:62F26978B84D02<5 | VFMADD231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=7 ; {sint16}. |000001B0:C4E2699ACB | VFMSUB132PS XMM1,XMM2,XMM3 |000001B5:C4E2699A4D40 | VFMSUB132PS XMM1,XMM2,[RBP+40h] |000001BB:62F26D0C9A4D04<4 | VFMSUB132PS XMM1,XMM2,[RBP+40h],MASK=K4 |000001C2:62F26D189A4D10<2 | VFMSUB132PS XMM1,XMM2,[RBP+40h],BCST=ON |000001C9:C4E26D9ACB | VFMSUB132PS YMM1,YMM2,YMM3 |000001CE:C4E26D9A4D40 | VFMSUB132PS YMM1,YMM2,[RBP+40h] |000001D4:62F26DAC9A4D02<5 | VFMSUB132PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000001DB:62F26D389A4D10<2 | VFMSUB132PS YMM1,YMM2,[RBP+40h],BCST=ON |000001E2:62F26D489ACB | VFMSUB132PS ZMM1,ZMM2,ZMM3 |000001E8:62F26D789ACB | VFMSUB132PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |000001EE:62F2691C9ACB | VFMSUB132PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; Swap inner pairs {cdab}. |000001F4:62F2699C9ACB | VFMSUB132PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; Round down. |000001FA:62F26D489A4D01<6 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h] |00000201:62F26DCC9A4D01<6 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000208:62F26D589A4D10<2 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],BCST=ON |0000020F:62F269089A4D01<6 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |00000216:62F269189A4D10<2 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |0000021D:62F269289A4D04<4 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000224:62F269389A4D02<5 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=3 ; {float16}. |0000022B:62F269489A4D04<4 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |00000232:62F269689A4D02<5 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=6 ; {uint16}. |00000239:62F269789A4D02<5 | VFMSUB132PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=7 ; {sint16}. |00000240:C4E269AACB | VFMSUB213PS XMM1,XMM2,XMM3 |00000245:C4E269AA4D40 | VFMSUB213PS XMM1,XMM2,[RBP+40h] |0000024B:62F26D0CAA4D04<4 | VFMSUB213PS XMM1,XMM2,[RBP+40h],MASK=K4 |00000252:62F26D18AA4D10<2 | VFMSUB213PS XMM1,XMM2,[RBP+40h],BCST=ON |00000259:C4E26DAACB | VFMSUB213PS YMM1,YMM2,YMM3 |0000025E:C4E26DAA4D40 | VFMSUB213PS YMM1,YMM2,[RBP+40h] |00000264:62F26DACAA4D02<5 | VFMSUB213PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000026B:62F26D38AA4D10<2 | VFMSUB213PS YMM1,YMM2,[RBP+40h],BCST=ON |00000272:62F26D48AACB | VFMSUB213PS ZMM1,ZMM2,ZMM3 |00000278:62F26D78AACB | VFMSUB213PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |0000027E:62F2691CAACB | VFMSUB213PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; Swap inner pairs {cdab}. |00000284:62F2699CAACB | VFMSUB213PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; Round down. |0000028A:62F26D48AA4D01<6 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h] |00000291:62F26DCCAA4D01<6 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000298:62F26D58AA4D10<2 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],BCST=ON |0000029F:62F26908AA4D01<6 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000002A6:62F26918AA4D10<2 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000002AD:62F26928AA4D04<4 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |000002B4:62F26938AA4D02<5 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=3 ; {float16}. |000002BB:62F26948AA4D04<4 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |000002C2:62F26968AA4D02<5 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=6 ; {uint16}. |000002C9:62F26978AA4D02<5 | VFMSUB213PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=7 ; {sint16}. |000002D0:C4E269BACB | VFMSUB231PS XMM1,XMM2,XMM3 |000002D5:C4E269BA4D40 | VFMSUB231PS XMM1,XMM2,[RBP+40h] |000002DB:62F26D0CBA4D04<4 | VFMSUB231PS XMM1,XMM2,[RBP+40h],MASK=K4 |000002E2:62F26D18BA4D10<2 | VFMSUB231PS XMM1,XMM2,[RBP+40h],BCST=ON |000002E9:C4E26DBACB | VFMSUB231PS YMM1,YMM2,YMM3 |000002EE:C4E26DBA4D40 | VFMSUB231PS YMM1,YMM2,[RBP+40h] |000002F4:62F26DACBA4D02<5 | VFMSUB231PS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000002FB:62F26D38BA4D10<2 | VFMSUB231PS YMM1,YMM2,[RBP+40h],BCST=ON |00000302:62F26D48BACB | VFMSUB231PS ZMM1,ZMM2,ZMM3 |00000308:62F26D78BACB | VFMSUB231PS ZMM1,ZMM2,ZMM3,ROUND=ZERO |0000030E:62F2691CBACB | VFMSUB231PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=1 ; Swap inner pairs {cdab}. |00000314:62F2699CBACB | VFMSUB231PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=1 ; Round down. |0000031A:62F26D48BA4D01<6 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h] |00000321:62F26DCCBA4D01<6 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000328:62F26D58BA4D10<2 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],BCST=ON |0000032F:62F26908BA4D01<6 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |00000336:62F26918BA4D10<2 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |0000033D:62F26928BA4D04<4 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000344:62F26938BA4D02<5 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=3 ; {float16}. |0000034B:62F26948BA4D04<4 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |00000352:62F26968BA4D02<5 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=6 ; {uint16}. |00000359:62F26978BA4D02<5 | VFMSUB231PS ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=7 ; {sint16}. |00000360:62F2699CA4CB | VFMADD233PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,ROUND=DOWN,SAE=OFF |00000366:62F269DCA4CB | VFMADD233PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,ROUND=DOWN,SAE=ON |0000036C:62F269DCA4CB | VFMADD233PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=1,OPER=5 |00000372:62F2690CA4CB | VFMADD233PS ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=0 |00000378:62F2690CA44D01<6 | VFMADD233PS ZMM1,ZMM2,[RBP+40h],MASK=K4 |0000037F:62F2690CA44D01<6 | VFMADD233PS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=0 ; {16to16}. |00000386:62F2692CA44D04<4 | VFMADD233PS ZMM1,ZMM2,[RBP+40h],MASK=K4,OPER=2 ; {4to16}. | |ENDPROGRAM t5410`

Expected messages t5410.out
  `I0180 Assembling source file "t5410.htm". I0270 Assembling source "t5410". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5410". "t5410.htm"{67} I0510 Assembling program pass 1. "t5410.htm"{67} I0530 Assembling program pass 2 - final. "t5410.htm"{67} I0660 16bit TINY BIN file "t5410.bin" created, size=909. "t5410.htm"{208} I0650 Program "t5410" assembled in 2 passes with errorlevel 0. "t5410.htm"{208} I0750 Source "t5410" (226 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5410.htm.lst" created, size=12023. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲