| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5256: Machine instructions VPBLENDW VPBLENDD VBLENDPS VBLENDPD

Tested procedures
  IiyVPBLENDW IiyVPBLENDD IiyVBLENDPS IiyVBLENDPD

Source & expected listing t5256.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=26,CPU=X64,SIMD=AVX2 | |t5256 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E3690ECB04 | VPBLENDW XMM1,XMM2,XMM3,4 |00000006:C4E36D0ECB04 | VPBLENDW YMM1,YMM2,YMM3,4 |0000000C:C4E3690E0E04 | VPBLENDW XMM1,XMM2,[RSI],4 |00000012:C4E36D0E0E04 | VPBLENDW YMM1,YMM2,[RSI],4 |00000018:C4E36902CB04 | VPBLENDD XMM1,XMM2,XMM3,4 |0000001E:C4E36D02CB04 | VPBLENDD YMM1,YMM2,YMM3,4 |00000024:C4E369020E04 | VPBLENDD XMM1,XMM2,[RSI],4 |0000002A:C4E36D020E04 | VPBLENDD YMM1,YMM2,[RSI],4 |00000030:C4E3690CCB04 | VBLENDPS XMM1,XMM2,XMM3,4 |00000036:C4E36D0CCB04 | VBLENDPS YMM1,YMM2,YMM3,4 |0000003C:C4E3690C0E04 | VBLENDPS XMM1,XMM2,[RSI],4 |00000042:C4E36D0C0E04 | VBLENDPS YMM1,YMM2,[RSI],4 |00000048:C4E3690DCB04 | VBLENDPD XMM1,XMM2,XMM3,4 |0000004E:C4E36D0DCB04 | VBLENDPD YMM1,YMM2,YMM3,4 |00000054:C4E3690D0E04 | VBLENDPD XMM1,XMM2,[RSI],4 |0000005A:C4E36D0D0E04 | VBLENDPD YMM1,YMM2,[RSI],4 | |ENDPROGRAM t5256`

Expected messages t5256.out
  `I0180 Assembling source file "t5256.htm". I0270 Assembling source "t5256". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5256". "t5256.htm"{58} I0510 Assembling program pass 1. "t5256.htm"{58} I0530 Assembling program pass 2 - final. "t5256.htm"{58} I0660 16bit TINY BIN file "t5256.bin" created, size=96. "t5256.htm"{76} I0650 Program "t5256" assembled in 2 passes with errorlevel 0. "t5256.htm"{76} I0750 Source "t5256" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5256.htm.lst" created, size=1146. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲