| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4524: Machine instructions VPMADCSSWD VPMADCSWD VPPERM VPCMOV

Tested procedures
  IixVPMADCSSWD IixVPMADCSWD IixVPPERM IixVPCMOV

Source & expected listing t4524.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,SIMD=AVX,AMD=ON,XOP=ON,PROT=ON | |t4524 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:8FE868A6CB40 | VPMADCSSWD XMM1,XMM2,XMM3,XMM4 |00000006:8FE868A60E40 | VPMADCSSWD XMM1,XMM2,[RSI],XMM4 |0000000C:8FE868B6CB40 | VPMADCSWD XMM1,XMM2,XMM3,XMM4 |00000012:8FE868B60E40 | VPMADCSWD XMM1,XMM2,[RSI],XMM4 |00000018:8FE868A30E40 | VPPERM XMM1,XMM2,[RSI],XMM4 |0000001E:8FE8E8A30E30 | VPPERM XMM1,XMM2,XMM3,[RSI] |00000024:8FE868A3CB40 | VPPERM XMM1,XMM2,XMM3,XMM4 |0000002A:8FE8E8A3CC30 | VPPERM XMM1,XMM2,XMM3,XMM4,CODE=LONG |00000030:8FE868A20E40 | VPCMOV XMM1,XMM2,[RSI],XMM4 |00000036:8FE8E8A20E30 | VPCMOV XMM1,XMM2,XMM3,[RSI] |0000003C:8FE868A2CB40 | VPCMOV XMM1,XMM2,XMM3,XMM4 |00000042:8FE8E8A2CC30 | VPCMOV XMM1,XMM2,XMM3,XMM4,CODE=LONG |00000048:8FE86CA20E40 | VPCMOV YMM1,YMM2,[RSI],YMM4 |0000004E:8FE8ECA20E30 | VPCMOV YMM1,YMM2,YMM3,[RSI] |00000054:8FE86CA2CB40 | VPCMOV YMM1,YMM2,YMM3,YMM4 |0000005A:8FE8ECA2CC30 | VPCMOV YMM1,YMM2,YMM3,YMM4,CODE=LONG | |ENDPROGRAM t4524`

Expected messages t4524.out
  `I0180 Assembling source file "t4524.htm". I0270 Assembling source "t4524". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4524". "t4524.htm"{58} I0510 Assembling program pass 1. "t4524.htm"{58} I0530 Assembling program pass 2 - final. "t4524.htm"{58} I0660 16bit TINY BIN file "t4524.bin" created, size=96. "t4524.htm"{76} I0650 Program "t4524" assembled in 2 passes with errorlevel 0. "t4524.htm"{76} I0750 Source "t4524" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4524.htm.lst" created, size=1272. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲