| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t2866: Pseudoinstruction %SETL

Tested procedures
  PseudopcSETL

Source & expected listing t2866.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPALL=YES,DUMPWIDTH=24, \ | | AUTOALIGN=OFF,LISTVAR=OFF | |t2866 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF | | %Var0 %SET ; Assigned nothing. |30 | %Len0 %SETL %Var0 ; Expected 0. |4142 | %Var1 %SET AB ; Assigned 1 operand. |31 | %Len1 %SETL %Var1 ; Expected 1. |2243442C454622 | %Var2 %SET "CD,EF" ; Assigned 1 operand. |31 | %Len2 %SETL %Var2 ; Expected 1. |47482C494A2C4B4C4D | %Var3 %SET GH, IJ, \ ; Assigned 3 operands. | | KLM |33 | %Len3 %SETL %Var3 ; Expected 3. |312C2C332C34 | %Var4 %SET 1,,3,4,,, ; Assigned 4 operands followed with empty ones. |34 | %Len4 %SETL %Var4 ; Expected 4. | |ENDPROGRAM t2866`

Expected messages t2866.out
  `I0180 Assembling source file "t2866.htm". I0270 Assembling source "t2866". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t2866". "t2866.htm"{50} I0510 Assembling program pass 1. "t2866.htm"{50} I0530 Assembling program pass 2 - final. "t2866.htm"{50} I0660 16bit TINY BIN file "t2866.bin" created, size=0. "t2866.htm"{62} I0650 Program "t2866" assembled in 2 passes with errorlevel 0. "t2866.htm"{62} I0750 Source "t2866" (80 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t2866.htm.lst" created, size=995. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲