| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3123: Machine instructions SBB SBBB SBBW SBBD SBBQ in 64bit mode

Tested procedures
  IigSBB IigSBBB IigSBBW IigSBBD IigSBBQ

Source & expected listing t3123.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=X64 | |t3123 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:1C02 | SBB AL,2 |00000002:80D802 | SBB AL,2,CODE=LONG |00000005:661D0200 | SBB AX,2 |00000009:6683D802 | SBB AX,2,CODE=LONG |0000000D:83D802 | SBB EAX,2 |00000010:1D02000000 | SBB EAX,2,CODE=SHORT |00000015:4883D802 | SBB RAX,2 |00000019:481D02000000 | SBB RAX,2,CODE=SHORT |0000001F:80D902 | SBB CL,2 |00000022:801DD500000002 | SBB [MemByte],2 |00000029:6683D902 | SBB CX,2 |0000002D:6681D90200 | SBB CX,2,IMM=WORD |00000032:66831DC200000002 | SBB [MemWord],2 |0000003A:66811DB90000000200 | SBB [MemWord],2,IMM=WORD |00000043:48811DAE00000002000000 | SBBQ [MemWord],2,IMM=DWORD |0000004E:83D902 | SBB ECX,2 |00000051:81D902000000 | SBB ECX,2,IMM=DWORD |00000057:831D9A00000002 | SBB [MemDword],2 |0000005E:48831D8A00000002 | SBB [MemQword],2 |00000066:48811D7F00000002000000 | SBB [MemQword],2,IMM=DWORD |00000071:67801F02 | SBBB [EDI],2 |00000075:6667831F02 | SBBW [EDI],2 |0000007A:67831F02 | SBBD [EDI],2 |0000007E:6748831F02 | SBBQ [EDI],2 |00000083:6748811F02000000 | SBBQ [EDI],2,IMM=DWORD |0000008B:18D1 | SBB CL,DL |0000008D:1ACA | SBB CL,DL,CODE=LONG |0000008F:18F5 | SBB CH,DH |00000091:1AEE | SBB CH,DH,CODE=LONG |00000093:4018F5 | SBB BPL,SIL |00000096:401AEE | SBB BPL,SIL,CODE=LONG |00000099:6619D1 | SBB CX,DX |0000009C:661BCA | SBB CX,DX,CODE=LONG |0000009F:19D1 | SBB ECX,EDX |000000A1:1BCA | SBB ECX,EDX,CODE=LONG |000000A3:4819D1 | SBB RCX,RDX |000000A6:481BCA | SBB RCX,RDX,CODE=LONG |000000A9:4D19D1 | SBB R9,R10 |000000AC:4D1BCA | SBB R9,R10,CODE=LONG |000000AF:4C19D1 | SBB RCX,R10 |000000B2:491BCA | SBB RCX,R10,CODE=LONG |000000B5:1A0D43000000 | SBB CL,[MemByte] |000000BB:661B0D3A000000 | SBB CX,[MemWord] |000000C2:1B0D30000000 | SBB ECX,[MemDword] |000000C8:481B0D21000000 | SBB RCX,[MemQword] |000000CF:181529000000 | SBB [MemByte],DL |000000D5:66191520000000 | SBB [MemWord],DX |000000DC:191516000000 | SBB [MemDword],EDX |000000E2:48191507000000 | SBB [MemQword],RDX |000000E9:0F1F8000000000 | ALIGN QWORD |000000F0:0000000000000000 |MemQword D Q |000000F8:00000000 |MemDword D D |000000FC:0000 |MemWord D W |000000FE:00 |MemByte D B | |ENDPROGRAM t3123`

Expected messages t3123.out
  `I0180 Assembling source file "t3123.htm". I0270 Assembling source "t3123". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3123". "t3123.htm"{61} I0510 Assembling program pass 1. "t3123.htm"{61} I0510 Assembling program pass 2. "t3123.htm"{61} I0510 Assembling program pass 3. "t3123.htm"{61} I0530 Assembling program pass 4 - final. "t3123.htm"{61} I0660 16bit TINY BIN file "t3123.bin" created, size=255. "t3123.htm"{117} I0650 Program "t3123" assembled in 4 passes with errorlevel 0. "t3123.htm"{117} I0750 Source "t3123" (137 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3123.htm.lst" created, size=3233. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲