| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5658: Machine instructions VRSQRT14SS VRSQRT14SD VRSQRT14PS VRSQRT14PD

Tested procedures
  IiyVRSQRT14SS IiyVRSQRT14SD IiyVRSQRT14PS IiyVRSQRT14PD

Source & expected listing t5658.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5658 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F26D084FCB | VRSQRT14SS XMM1,XMM2,XMM3 |00000006:62F26D8C4FCB | VRSQRT14SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |0000000C:62F26D084F4D10<2 | VRSQRT14SS XMM1,XMM2,[RBP+40h] |00000013:62F26D8C4F4D10<2 | VRSQRT14SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000001A:62F2ED084FCB | VRSQRT14SD XMM1,XMM2,XMM3 |00000020:62F2ED8C4FCB | VRSQRT14SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000026:62F2ED084F4D08<3 | VRSQRT14SD XMM1,XMM2,[RBP+40h] |0000002D:62F2ED8C4F4D08<3 | VRSQRT14SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000034:62F27D8B4ECA | VRSQRT14PS XMM1,XMM2,MASK=K3,ZEROING=ON |0000003A:62F27DAB4ECA | VRSQRT14PS YMM1,YMM2,MASK=K3,ZEROING=ON |00000040:62F27DCB4ECA | VRSQRT14PS ZMM1,ZMM2,MASK=K3,ZEROING=ON |00000046:62F27D8B4E4D04<4 | VRSQRT14PS XMM1,[RBP+40h],MASK=K3,ZEROING=ON |0000004D:62F27DAB4E4D02<5 | VRSQRT14PS YMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000054:62F27DCB4E4D01<6 | VRSQRT14PS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |0000005B:62F27D9B4E4D10<2 | VRSQRT14PS XMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |00000062:62F27DBB4E4D10<2 | VRSQRT14PS YMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |00000069:62F27DDB4E4D10<2 | VRSQRT14PS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |00000070:62F2FD8B4ECA | VRSQRT14PD XMM1,XMM2,MASK=K3,ZEROING=ON |00000076:62F2FDAB4ECA | VRSQRT14PD YMM1,YMM2,MASK=K3,ZEROING=ON |0000007C:62F2FDCB4ECA | VRSQRT14PD ZMM1,ZMM2,MASK=K3,ZEROING=ON |00000082:62F2FD8B4E4D04<4 | VRSQRT14PD XMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000089:62F2FDAB4E4D02<5 | VRSQRT14PD YMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000090:62F2FDCB4E4D01<6 | VRSQRT14PD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000097:62F2FD9B4E4D08<3 | VRSQRT14PD XMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |0000009E:62F2FDBB4E4D08<3 | VRSQRT14PD YMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |000000A5:62F2FDDB4E4D08<3 | VRSQRT14PD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON | |ENDPROGRAM t5658`

Expected messages t5658.out
  `I0180 Assembling source file "t5658.htm". I0270 Assembling source "t5658". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5658". "t5658.htm"{58} I0510 Assembling program pass 1. "t5658.htm"{58} I0530 Assembling program pass 2 - final. "t5658.htm"{58} I0660 16bit TINY BIN file "t5658.bin" created, size=172. "t5658.htm"{86} I0650 Program "t5658" assembled in 2 passes with errorlevel 0. "t5658.htm"{86} I0750 Source "t5658" (104 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5658.htm.lst" created, size=2264. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲