| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5636: Machine instructions VPSLLVW VPSLLVD VPSLLVQ

Tested procedures
  IizVPSLLVW IizVPSLLVD IizVPSLLVQ

Source & expected listing t5636.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5636 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2ED0812CB | VPSLLVW XMM1,XMM2,XMM3 |00000006:62F2ED2C12CB | VPSLLVW YMM1,YMM2,YMM3,MASK=K4 |0000000C:62F2EDCC12CB | VPSLLVW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000012:62F2ED08124D04<4 | VPSLLVW XMM1,XMM2,[RBP+40h] |00000019:62F2ED2C124D02<5 | VPSLLVW YMM1,YMM2,[RBP+40h],MASK=K4 |00000020:62F2EDCC124D01<6 | VPSLLVW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000027:C4E26947CB | VPSLLVD XMM1,XMM2,XMM3 |0000002C:C4E26D47CB | VPSLLVD YMM1,YMM2,YMM3 |00000031:62F26D0C47CB | VPSLLVD XMM1,XMM2,XMM3,MASK=K4 |00000037:62F26D2C47CB | VPSLLVD YMM1,YMM2,YMM3,MASK=K4 |0000003D:62F26D4847CB | VPSLLVD ZMM1,ZMM2,ZMM3 |00000043:62F2692847CB | VPSLLVD ZMM1,ZMM2,ZMM3,EH=OFF,OPER=2 ; MVEX {badc}. |00000049:C4E269474D40 | VPSLLVD XMM1,XMM2,[RBP+40h] |0000004F:C4E26D474D40 | VPSLLVD YMM1,YMM2,[RBP+40h] |00000055:62F26D08474D04<4 | VPSLLVD XMM1,XMM2,[RBP+40h],BCST=OFF |0000005C:62F26D28474D02<5 | VPSLLVD YMM1,YMM2,[RBP+40h],BCST=OFF |00000063:62F26D48474D01<6 | VPSLLVD ZMM1,ZMM2,[RBP+40h],BCST=OFF |0000006A:62F26D18474D10<2 | VPSLLVD XMM1,XMM2,[RBP+40h],BCST=ON |00000071:62F26D38474D10<2 | VPSLLVD YMM1,YMM2,[RBP+40h],BCST=ON |00000078:62F26D58474D10<2 | VPSLLVD ZMM1,ZMM2,[RBP+40h],BCST=ON |0000007F:62F26908474D01<6 | VPSLLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |00000086:62F26918474D10<2 | VPSLLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |0000008D:62F26928474D04<4 | VPSLLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000094:62F26948474D04<4 | VPSLLVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |0000009B:C4E2E947CB | VPSLLVQ XMM1,XMM2,XMM3 |000000A0:C4E2ED47CB | VPSLLVQ YMM1,YMM2,YMM3 |000000A5:62F2ED0C47CB | VPSLLVQ XMM1,XMM2,XMM3,MASK=K4 |000000AB:62F2ED2C47CB | VPSLLVQ YMM1,YMM2,YMM3,MASK=K4 |000000B1:62F2ED4847CB | VPSLLVQ ZMM1,ZMM2,ZMM3 |000000B7:C4E2E9474D40 | VPSLLVQ XMM1,XMM2,[RBP+40h] |000000BD:C4E2ED474D40 | VPSLLVQ YMM1,YMM2,[RBP+40h] |000000C3:62F2ED0C474D04<4 | VPSLLVQ XMM1,XMM2,[RBP+40h],MASK=K4 |000000CA:62F2ED2C474D02<5 | VPSLLVQ YMM1,YMM2,[RBP+40h],MASK=K4 |000000D1:62F2ED48474D01<6 | VPSLLVQ ZMM1,ZMM2,[RBP+40h] | |ENDPROGRAM t5636`

Expected messages t5636.out
  `I0180 Assembling source file "t5636.htm". I0270 Assembling source "t5636". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5636". "t5636.htm"{55} I0510 Assembling program pass 1. "t5636.htm"{55} I0530 Assembling program pass 2 - final. "t5636.htm"{55} I0660 16bit TINY BIN file "t5636.bin" created, size=216. "t5636.htm"{91} I0650 Program "t5636" assembled in 2 passes with errorlevel 0. "t5636.htm"{91} I0750 Source "t5636" (109 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5636.htm.lst" created, size=2581. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲