| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3845: Machine instructions CVTDQ2PD CVTPD2DQ CVTPD2PS CVTPS2DQ CVTSD2SS CVTSS2SD CVTTPD2DQ CVTTPS2DQ

Tested procedures
  IipGroupSSE IipCVTDQ2PD IipCVTPD2DQ IipCVTPD2PS IipCVTPS2DQ IipCVTSD2SS IipCVTSS2SD IipCVTTPD2DQ IipCVTTPS2DQ

Source & expected listing t3845.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE2 | |t3845 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:F30FE6CF | CVTDQ2PD XMM1,XMM7 |0004:F30FE60C | CVTDQ2PD XMM1,[SI] |0008:F20FE6CF | CVTPD2DQ XMM1,XMM7 |000C:F20FE60C | CVTPD2DQ XMM1,[SI] |0010:660F5ACF | CVTPD2PS XMM1,XMM7 |0014:660F5A0C | CVTPD2PS XMM1,[SI] |0018:660F5BCF | CVTPS2DQ XMM1,XMM7 |001C:660F5B0C | CVTPS2DQ XMM1,[SI] |0020:F20F5ACF | CVTSD2SS XMM1,XMM7 |0024:F20F5A0C | CVTSD2SS XMM1,[SI] |0028:F30F5ACF | CVTSS2SD XMM1,XMM7 |002C:F30F5A0C | CVTSS2SD XMM1,[SI] |0030:660FE6CF | CVTTPD2DQ XMM1,XMM7 |0034:660FE60C | CVTTPD2DQ XMM1,[SI] |0038:F30F5BCF | CVTTPS2DQ XMM1,XMM7 |003C:F30F5B0C | CVTTPS2DQ XMM1,[SI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:F30FE6CF | CVTDQ2PD XMM1,XMM7 |00000004:F30FE60E | CVTDQ2PD XMM1,[ESI] |00000008:F20FE6CF | CVTPD2DQ XMM1,XMM7 |0000000C:F20FE60E | CVTPD2DQ XMM1,[ESI] |00000010:660F5ACF | CVTPD2PS XMM1,XMM7 |00000014:660F5A0E | CVTPD2PS XMM1,[ESI] |00000018:660F5BCF | CVTPS2DQ XMM1,XMM7 |0000001C:660F5B0E | CVTPS2DQ XMM1,[ESI] |00000020:F20F5ACF | CVTSD2SS XMM1,XMM7 |00000024:F20F5A0E | CVTSD2SS XMM1,[ESI] |00000028:F30F5ACF | CVTSS2SD XMM1,XMM7 |0000002C:F30F5A0E | CVTSS2SD XMM1,[ESI] |00000030:660FE6CF | CVTTPD2DQ XMM1,XMM7 |00000034:660FE60E | CVTTPD2DQ XMM1,[ESI] |00000038:F30F5BCF | CVTTPS2DQ XMM1,XMM7 |0000003C:F30F5B0E | CVTTPS2DQ XMM1,[ESI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:F3450FE6CB | CVTDQ2PD XMM9,XMM11 |00000005:F3440FE60E | CVTDQ2PD XMM9,[RSI] |0000000A:F20FE6CF | CVTPD2DQ XMM1,XMM7 |0000000E:67F20FE60E | CVTPD2DQ XMM1,[ESI] |00000013:660F5ACF | CVTPD2PS XMM1,XMM7 |00000017:660F5A0C2500000000 | CVTPD2PS XMM1,[0] |00000020:660F5BCF | CVTPS2DQ XMM1,XMM7 |00000024:6667460F5B5C4DF6 | CVTPS2DQ XMM11,[2*R9D+EBP-10] |0000002C:F2410F5ACB | CVTSD2SS XMM1,XMM11 |00000031:F2410F5A09 | CVTSD2SS XMM1,[R9] |00000036:F3410F5ACB | CVTSS2SD XMM1,XMM11 |0000003B:F3410F5A09 | CVTSS2SD XMM1,[R9] |00000040:660FE6CF | CVTTPD2DQ XMM1,XMM7 |00000044:6466670FE60E | CVTTPD2DQ XMM1,[FS:ESI] |0000004A:F3440F5BCF | CVTTPS2DQ XMM9,XMM7 |0000004F:F3440F5B0E | CVTTPS2DQ XMM9,[RSI] | |ENDPROGRAM t3845`

Expected messages t3845.out
  `I0180 Assembling source file "t3845.htm". I0270 Assembling source "t3845". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3845". "t3845.htm"{73} I0510 Assembling program pass 1. "t3845.htm"{73} I0530 Assembling program pass 2 - final. "t3845.htm"{73} I0660 16bit TINY BIN file "t3845.bin" created, size=212. "t3845.htm"{125} I0650 Program "t3845" assembled in 2 passes with errorlevel 0. "t3845.htm"{125} I0750 Source "t3845" (143 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3845.htm.lst" created, size=3037. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲