| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3215: Machine instructions INS INSB INSW INSD

Tested procedures
  IigINS IigINSB IigINSW IigINSD

Source & expected listing t3215.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, PRIV=ENABLED | |t3215 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF | |;; |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:6C | INSB |0001:6D | INSW |0002:666D | INSD |0004:6C | INS DATA=BYTE |0005:6D | INS DATA=WORD |0006:666D | INS DATA=DWORD |0008:F36D | REP INSW |000A:F36D | REPE INSW |000C:F26D | REPNE INSW |000E:6D | INSW [DI] |000F:6D | INSW [DI],DX |0010:676D | INSW [EDI] |0012:676D | INSW [ES:EDI] |0014:6D | INSW [ES:DI] |0015:266D | SEGES INSW |0017:6C | INS [MemByte] |0018:6D | INS [MemWord] |0019:666D | INS [MemDword] |001B:6D | INS [MemQword],DATA=WORD |001C:6C | INS [DI+MemByte] |001D:6D | INS [DI+MemWord] |001E:666D | INS [DI+MemDword] | |;; |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:6C | INSB |00000001:666D | INSW |00000003:6D | INSD |00000004:6C | INS DATA=BYTE |00000005:666D | INS DATA=WORD |00000007:6D | INS DATA=DWORD |00000008:F3666D | REP INSW |0000000B:F3666D | REPE INSW |0000000E:F2666D | REPNE INSW |00000011:676D | INSD [DI] |00000013:6D | INSD [EDI] |00000014:6D | INSD [EDI],DX |00000015:6D | INSD [ES:EDI] |00000016:266D | SEGES INSD [EDI] |00000018:6C | INS [MemByte] |00000019:666D | INS [MemWord] |0000001B:6D | INS [MemDword] |0000001C:6D | INS [MemQword],DATA=DWORD |0000001D:6C | INS [EDI+MemByte] |0000001E:666D | INS [EDI+MemWord] |00000020:6D | INS [EDI+MemDword] | |;; |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:6C | INSB |00000001:666D | INSW |00000003:6D | INSD |00000004:6C | INS DATA=BYTE |00000005:666D | INS DATA=WORD |00000007:6D | INS DATA=DWORD |00000008:6D | INSD [RDI] |00000009:6D | INSD [RDI],DX |0000000A:676D | INSD [EDI] |0000000C:676D | INSD [ES:EDI] |0000000E:6D | INSD [ES:RDI] |0000000F:266D | SEGES INSD |00000011:6C | INS [MemByte] |00000012:666D | INS [MemWord] |00000014:6D | INS [MemDword] |00000015:6D | INS [MemQword] |00000016:6C | INS [MemByte] |00000017:666D | INS [MemWord] |00000019:6D | INS [MemDword] |0000001A:6D | INS [MemQword] |0000001B:0F1F442000 | ALIGN QWORD |00000020:0000000000000000 |MemQword DQ Q |00000028:00000000 |MemDword DD D |0000002C:0000 |MemWord DW W |0000002E:00 |MemByte DB B | | ENDPROGRAM t3215`

Expected messages t3215.out
  `I0180 Assembling source file "t3215.htm". I0270 Assembling source "t3215". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3215". "t3215.htm"{58} I0510 Assembling program pass 1. "t3215.htm"{58} I0510 Assembling program pass 2. "t3215.htm"{58} I0510 Assembling program pass 3. "t3215.htm"{58} I0530 Assembling program pass 4 - final. "t3215.htm"{58} I0660 16bit TINY BIN file "t3215.bin" created, size=127. "t3215.htm"{133} I0650 Program "t3215" assembled in 4 passes with errorlevel 0. "t3215.htm"{133} I0750 Source "t3215" (153 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3215.htm.lst" created, size=3588. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲