| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5780: Machine instructions VPTERNLOGD VPTERNLOGQ VPALIGNR

Tested procedures
  IiyVPTERNLOGD IiyVPTERNLOGQ IiyVPALIGNR

Source & expected listing t5780.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5780 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F36D8D25CB04 | VPTERNLOGD XMM1,XMM2,XMM3,4,MASK=K5, ZEROING=ON |00000007:62F36DAD25CB04 | VPTERNLOGD YMM1,YMM2,YMM3,4,MASK=K5, ZEROING=ON |0000000E:62F36DCD25CB04 | VPTERNLOGD ZMM1,ZMM2,ZMM3,4,MASK=K5, ZEROING=ON |00000015:62F36D8D254D04<404 | VPTERNLOGD XMM1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |0000001D:62F36DAD254D02<504 | VPTERNLOGD YMM1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |00000025:62F36DCD254D01<604 | VPTERNLOGD ZMM1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |0000002D:62F36D9D254D10<204 | VPTERNLOGD XMM1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |00000035:62F36DBD254D10<204 | VPTERNLOGD YMM1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |0000003D:62F36DDD254D10<204 | VPTERNLOGD ZMM1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |00000045:62F3ED8D25CB04 | VPTERNLOGQ XMM1,XMM2,XMM3,4,MASK=K5, ZEROING=ON |0000004C:62F3EDAD25CB04 | VPTERNLOGQ YMM1,YMM2,YMM3,4,MASK=K5, ZEROING=ON |00000053:62F3EDCD25CB04 | VPTERNLOGQ ZMM1,ZMM2,ZMM3,4,MASK=K5, ZEROING=ON |0000005A:62F3ED8D254D04<404 | VPTERNLOGQ XMM1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |00000062:62F3EDAD254D02<504 | VPTERNLOGQ YMM1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |0000006A:62F3EDCD254D01<604 | VPTERNLOGQ ZMM1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |00000072:62F3ED9D254D08<304 | VPTERNLOGQ XMM1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |0000007A:62F3EDBD254D08<304 | VPTERNLOGQ YMM1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |00000082:62F3EDDD254D08<304 | VPTERNLOGQ ZMM1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON,BCST=ON |0000008A:C4E3690FCB04 | VPALIGNR XMM1,XMM2,XMM3,4 |00000090:C4E36D0FCB04 | VPALIGNR YMM1,YMM2,YMM3,4 |00000096:62F36D8D0FCB04 | VPALIGNR XMM1,XMM2,XMM3,4,MASK=K5,ZEROING=ON |0000009D:62F36DAD0FCB04 | VPALIGNR YMM1,YMM2,YMM3,4,MASK=K5,ZEROING=ON |000000A4:62F36DCD0FCB04 | VPALIGNR ZMM1,ZMM2,ZMM3,4,MASK=K5,ZEROING=ON |000000AB:C4E3690F4D4004 | VPALIGNR XMM1,XMM2,[RBP+40h],4 |000000B2:C4E36D0F4D4004 | VPALIGNR YMM1,YMM2,[RBP+40h],4 |000000B9:62F36D8D0F4D04<404 | VPALIGNR XMM1,XMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000C1:62F36DAD0F4D02<504 | VPALIGNR YMM1,YMM2,[RBP+40h],4,MASK=K5,ZEROING=ON |000000C9:62F36DCD0F4D01<604 | VPALIGNR ZMM1,ZMM2,[RBP+40h],4,MASK=K5,ZEROING=ON | |ENDPROGRAM t5780`

Expected messages t5780.out
  `I0180 Assembling source file "t5780.htm". I0270 Assembling source "t5780". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5780". "t5780.htm"{55} I0510 Assembling program pass 1. "t5780.htm"{55} I0530 Assembling program pass 2 - final. "t5780.htm"{55} I0660 16bit TINY BIN file "t5780.bin" created, size=209. "t5780.htm"{85} I0650 Program "t5780" assembled in 2 passes with errorlevel 0. "t5780.htm"{85} I0750 Source "t5780" (103 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5780.htm.lst" created, size=2564. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲