| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5710: Machine instructions VSCALEFSS VSCALEFSD VSCALEFPS VSCALEFPD VSCALEPS

Tested procedures
  IiyVSCALEFSS IiyVSCALEFSD IiyVSCALEFPS IiyVSCALEFPD IiyVSCALEPS

Source & expected listing t5710.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=28, CPU=X64, SIMD=AVX512,EVEX=ON | |t5710 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F26D082DCB | VSCALEFSS XMM1,XMM2,XMM3 |00000006:62F26DDC2DCB | VSCALEFSS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON,ROUND=UP |0000000C:62F26D082D4D10<2 | VSCALEFSS XMM1,XMM2,[RBP+40h] |00000013:62F26D8C2D4D10<2 | VSCALEFSS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000001A:62F2ED082DCB | VSCALEFSD XMM1,XMM2,XMM3 |00000020:62F2EDDC2DCB | VSCALEFSD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON,ROUND=UP |00000026:62F2ED082D4D08<3 | VSCALEFSD XMM1,XMM2,[RBP+40h] |0000002D:62F2ED8C2D4D08<3 | VSCALEFSD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000034:62F26D082CCB | VSCALEFPS XMM1,XMM2,XMM3 |0000003A:62F26D282CCB | VSCALEFPS YMM1,YMM2,YMM3 |00000040:62F26D482CCB | VSCALEFPS ZMM1,ZMM2,ZMM3 |00000046:62F26D8C2CCB | VSCALEFPS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |0000004C:62F26DAC2CCB | VSCALEFPS YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000052:62F26DBC2CCB | VSCALEFPS ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON,ROUND=DOWN |00000058:62F26D082C4D04<4 | VSCALEFPS XMM1,XMM2,[RBP+40h],BCST=OFF |0000005F:62F26D282C4D02<5 | VSCALEFPS YMM1,YMM2,[RBP+40h],BCST=OFF |00000066:62F26D482C4D01<6 | VSCALEFPS ZMM1,ZMM2,[RBP+40h],BCST=OFF |0000006D:62F26D182C4D10<2 | VSCALEFPS XMM1,XMM2,[RBP+40h],BCST=ON |00000074:62F26D382C4D10<2 | VSCALEFPS YMM1,YMM2,[RBP+40h],BCST=ON |0000007B:62F26D582C4D10<2 | VSCALEFPS ZMM1,ZMM2,[RBP+40h],BCST=ON |00000082:62F2ED082CCB | VSCALEFPD XMM1,XMM2,XMM3 |00000088:62F2ED282CCB | VSCALEFPD YMM1,YMM2,YMM3 |0000008E:62F2ED482CCB | VSCALEFPD ZMM1,ZMM2,ZMM3 |00000094:62F2ED8C2CCB | VSCALEFPD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |0000009A:62F2EDAC2CCB | VSCALEFPD YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |000000A0:62F2EDBC2CCB | VSCALEFPD ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON,ROUND=DOWN |000000A6:62F2ED082C4D04<4 | VSCALEFPD XMM1,XMM2,[RBP+40h],BCST=OFF |000000AD:62F2ED282C4D02<5 | VSCALEFPD YMM1,YMM2,[RBP+40h],BCST=OFF |000000B4:62F2ED482C4D01<6 | VSCALEFPD ZMM1,ZMM2,[RBP+40h],BCST=OFF |000000BB:62F2ED182C4D08<3 | VSCALEFPD XMM1,XMM2,[RBP+40h],BCST=ON |000000C2:62F2ED382C4D08<3 | VSCALEFPD YMM1,YMM2,[RBP+40h],BCST=ON |000000C9:62F2ED582C4D08<3 | VSCALEFPD ZMM1,ZMM2,[RBP+40h],BCST=ON | | EUROASM MVEX=ENABLED |000000D0:62F2699884CB | VSCALEPS ZMM1,ZMM2,ZMM3,ROUND=DOWN,SAE=OFF ; EH=1, OPER=1. |000000D6:62F269F884CB | VSCALEPS ZMM1,ZMM2,ZMM3,ROUND=ZERO,SAE=ON ; EH=1, OPER=7. |000000DC:62F269C884CB | VSCALEPS ZMM1,ZMM2,ZMM3,EH=1,OPER=4 ; ROUND=NEAR, SAE=ON. |000000E2:62F2692884CB | VSCALEPS ZMM1,ZMM2,ZMM3,EH=0,OPER=2 ; Swizzle {badc}. |000000E8:62F26908844D01<6 | VSCALEPS ZMM1,ZMM2,[RBP+40h],OPER=0 ; {16to16}. |000000EF:62F26918844D10<2 | VSCALEPS ZMM1,ZMM2,[RBP+40h],OPER=1 ; {1to16}. |000000F6:62F26928844D04<4 | VSCALEPS ZMM1,ZMM2,[RBP+40h],OPER=2 ; {4to16}. |000000FD:62F26978844D02<5 | VSCALEPS ZMM1,ZMM2,[RBP+40h],OPER=7 ; {sint16}. | |ENDPROGRAM t5710`

Expected messages t5710.out
  `I0180 Assembling source file "t5710.htm". I0270 Assembling source "t5710". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5710". "t5710.htm"{61} I0510 Assembling program pass 1. "t5710.htm"{61} I0530 Assembling program pass 2 - final. "t5710.htm"{61} I0660 16bit TINY BIN file "t5710.bin" created, size=260. "t5710.htm"{104} I0650 Program "t5710" assembled in 2 passes with errorlevel 0. "t5710.htm"{104} I0750 Source "t5710" (122 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5710.htm.lst" created, size=3181. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲