| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5748: Machine instructions VPERM2F128 VPERM2I128

Tested procedures
  IiyVPERM2F128 IiyVPERM2I128

Source & expected listing t5748.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512 | |t5748 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E36D06CB04 | VPERM2F128 YMM1,YMM2,YMM3,4 |00000006:C4E36D060E04 | VPERM2F128 YMM1,YMM2,[RSI],4 |0000000C:C4E36D46CB04 | VPERM2I128 YMM1,YMM2,YMM3,4 |00000012:C4E36D460E04 | VPERM2I128 YMM1,YMM2,[RSI],4 | |ENDPROGRAM t5748`

Expected messages t5748.out
  `I0180 Assembling source file "t5748.htm". I0270 Assembling source "t5748". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5748". "t5748.htm"{52} I0510 Assembling program pass 1. "t5748.htm"{52} I0530 Assembling program pass 2 - final. "t5748.htm"{52} I0660 16bit TINY BIN file "t5748.bin" created, size=24. "t5748.htm"{58} I0650 Program "t5748" assembled in 2 passes with errorlevel 0. "t5748.htm"{58} I0750 Source "t5748" (76 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5748.htm.lst" created, size=535. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲