| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4110: Machine instructions MONTMUL XSTORE XCRYPTECB XCRYPTCBC XCRYPTCTR XCRYPTCFB XCRYPTOFB XSHA1 XSHA256

Description
  VIA Nano Padlock cryptographic instructions.
Tested procedures
  IitGroupPadlock IitMONTMUL IitXSTORE IitXCRYPTECB IitXCRYPTCBC IitXCRYPTCTR IitXCRYPTCFB IitXCRYPTOFB IitXSHA1 IitXSHA256

Source & expected listing t4110.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=28, CPU=X64, CYRIX=ON, SPEC=ON | |t4110 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FA7C0 | XSTORE |0003:F30FA7C0 | REP XSTORE |0007:F30FA6C0 | MONTMUL |000B:F30FA6C0 | REP MONTMUL |000F:F30FA7C8 | XCRYPTECB |0013:F30FA7D0 | XCRYPTCBC |0017:F30FA7D8 | XCRYPTCTR |001B:F30FA7E0 | XCRYPTCFB |001F:F30FA7E8 | XCRYPTOFB |0023:F30FA6C8 | XSHA1 |0027:F30FA6D0 | XSHA256 |002B:F30FA6D0 | REP XSHA256 |002F:67F30FA6D0 | ATOGGLE XSHA256 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0FA7C0 | XSTORE |00000003:F30FA7C0 | REP XSTORE |00000007:F30FA6C0 | MONTMUL |0000000B:F30FA6C0 | REP MONTMUL |0000000F:F30FA7C8 | XCRYPTECB |00000013:F30FA7D0 | XCRYPTCBC |00000017:F30FA7D8 | XCRYPTCTR |0000001B:F30FA7E0 | XCRYPTCFB |0000001F:F30FA7E8 | XCRYPTOFB |00000023:F30FA6C8 | XSHA1 |00000027:F30FA6D0 | XSHA256 |0000002B:F30FA6D0 | REP XSHA256 |0000002F:67F30FA6D0 | ATOGGLE XSHA256 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0FA7C0 | XSTORE |00000003:F30FA7C0 | REP XSTORE |00000007:F30FA6C0 | MONTMUL |0000000B:F30FA6C0 | REP MONTMUL |0000000F:F30FA7C8 | XCRYPTECB |00000013:F30FA7D0 | XCRYPTCBC |00000017:F30FA7D8 | XCRYPTCTR |0000001B:F30FA7E0 | XCRYPTCFB |0000001F:F30FA7E8 | XCRYPTOFB |00000023:F30FA6C8 | XSHA1 |00000027:F30FA6D0 | XSHA256 |0000002B:F30FA6D0 | REP XSHA256 |0000002F:67F30FA6D0 | ATOGGLE XSHA256 | |ENDPROGRAM t4110`

Expected messages t4110.out
  `I0180 Assembling source file "t4110.htm". I0270 Assembling source "t4110". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4110". "t4110.htm"{79} I0510 Assembling program pass 1. "t4110.htm"{79} I0530 Assembling program pass 2 - final. "t4110.htm"{79} I0660 16bit TINY BIN file "t4110.bin" created, size=180. "t4110.htm"{122} I0650 Program "t4110" assembled in 2 passes with errorlevel 0. "t4110.htm"{122} I0750 Source "t4110" (140 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4110.htm.lst" created, size=2009. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲