| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3570: Machine instructions FNSAVE, FSAVE, FRSTOR, FXSAVE, FXSAVE64, FXRSTOR, FXRSTOR64

Tested procedures
  IifFNSAVE IifFSAVE IifFRSTOR IifFXSAVE IifFXSAVE64 IifFXRSTOR IifFXRSTOR64

Source & expected listing t3570.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32,CPU=086, SIMD=SSE, FPU=ON, MMX=ON | |t3570 PROGRAM FORMAT=BIN, WIDTH=16, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:DD36[3100] | FNSAVE [Env] |0004:9BDD36[3100] | FSAVE [Env] |0009:DD26[3100] | FRSTOR [Env] | | EUROASM CPU=686 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:DD35[31000000] | FNSAVE [Env] |00000006:9BDD35[31000000] | FSAVE [Env] |0000000D:DD25[31000000] | FRSTOR [Env] |00000013:0FAE05[31000000] | FXSAVE [Env] |0000001A:0FAE0D[31000000] | FXRSTOR [Env] | | EUROASM CPU=X64 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:DD352B000000 | FNSAVE [Env] |00000006:9BDD3524000000 | FSAVE [Env] |0000000D:DD251E000000 | FRSTOR [Env] |00000013:0FAE0517000000 | FXSAVE [Env] |0000001A:480FAE050F000000 | FXSAVE64 [Env] |00000022:0FAE0D08000000 | FXRSTOR [Env] |00000029:480FAE0D00000000 | FXRSTOR64 [Env] |00000031: |Env: | | ENDPROGRAM t3570`

Expected messages t3570.out
  `I0180 Assembling source file "t3570.htm". I0270 Assembling source "t3570". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3570". "t3570.htm"{67} I0510 Assembling program pass 1. "t3570.htm"{67} I0510 Assembling program pass 2. "t3570.htm"{67} I0530 Assembling program pass 3 - final. "t3570.htm"{67} I0660 16bit TINY BIN file "t3570.bin" created, size=113. "t3570.htm"{89} I0650 Program "t3570" assembled in 3 passes with errorlevel 0. "t3570.htm"{89} I0750 Source "t3570" (108 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3570.htm.lst" created, size=1345. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲