| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5610: Machine instructions VHADDPS VHADDPD VHSUBPS VHSUBPD

Tested procedures
  IizVHADDPS IizVHADDPD IizVHSUBPS IizVHSUBPD

Source & expected listing t5610.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=26,CPU=X64,SIMD=AVX | |t5610 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5EB7CCB | VHADDPS XMM1,XMM2,XMM3 |00000004:C5EF7CCB | VHADDPS YMM1,YMM2,YMM3 |00000008:C4E16B7CCB | VHADDPS XMM1,XMM2,XMM3,PREFIX=VEX3 |0000000D:C4E16F7CCB | VHADDPS YMM1,YMM2,YMM3,PREFIX=VEX3 |00000012:C5EB7C4D40 | VHADDPS XMM1,XMM2,[RBP+40h] |00000017:C5EF7C4D40 | VHADDPS YMM1,YMM2,[RBP+40h] |0000001C:C4E16B7C4D40 | VHADDPS XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000022:C4E16F7C4D40 | VHADDPS YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |00000028:C5E97CCB | VHADDPD XMM1,XMM2,XMM3 |0000002C:C5ED7CCB | VHADDPD YMM1,YMM2,YMM3 |00000030:C4E1697CCB | VHADDPD XMM1,XMM2,XMM3,PREFIX=VEX3 |00000035:C4E16D7CCB | VHADDPD YMM1,YMM2,YMM3,PREFIX=VEX3 |0000003A:C5E97C4D40 | VHADDPD XMM1,XMM2,[RBP+40h] |0000003F:C5ED7C4D40 | VHADDPD YMM1,YMM2,[RBP+40h] |00000044:C4E1697C4D40 | VHADDPD XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |0000004A:C4E16D7C4D40 | VHADDPD YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |00000050:C5EB7DCB | VHSUBPS XMM1,XMM2,XMM3 |00000054:C5EF7DCB | VHSUBPS YMM1,YMM2,YMM3 |00000058:C4E16B7DCB | VHSUBPS XMM1,XMM2,XMM3,PREFIX=VEX3 |0000005D:C4E16F7DCB | VHSUBPS YMM1,YMM2,YMM3,PREFIX=VEX3 |00000062:C5EB7D4D40 | VHSUBPS XMM1,XMM2,[RBP+40h] |00000067:C5EF7D4D40 | VHSUBPS YMM1,YMM2,[RBP+40h] |0000006C:C4E16B7D4D40 | VHSUBPS XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000072:C4E16F7D4D40 | VHSUBPS YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |00000078:C5E97DCB | VHSUBPD XMM1,XMM2,XMM3 |0000007C:C5ED7DCB | VHSUBPD YMM1,YMM2,YMM3 |00000080:C4E1697DCB | VHSUBPD XMM1,XMM2,XMM3,PREFIX=VEX3 |00000085:C4E16D7DCB | VHSUBPD YMM1,YMM2,YMM3,PREFIX=VEX3 |0000008A:C5E97D4D40 | VHSUBPD XMM1,XMM2,[RBP+40h] |0000008F:C5ED7D4D40 | VHSUBPD YMM1,YMM2,[RBP+40h] |00000094:C4E1697D4D40 | VHSUBPD XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |0000009A:C4E16D7D4D40 | VHSUBPD YMM1,YMM2,[RBP+40h],PREFIX=VEX3 | |ENDPROGRAM t5610`

Expected messages t5610.out
  `I0180 Assembling source file "t5610.htm". I0270 Assembling source "t5610". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5610". "t5610.htm"{58} I0510 Assembling program pass 1. "t5610.htm"{58} I0530 Assembling program pass 2 - final. "t5610.htm"{58} I0660 16bit TINY BIN file "t5610.bin" created, size=160. "t5610.htm"{92} I0650 Program "t5610" assembled in 2 passes with errorlevel 0. "t5610.htm"{92} I0750 Source "t5610" (110 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5610.htm.lst" created, size=2177. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲