| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3439: Machine instructions LOADALL LOADALL286

Tested procedures
  IisLOADALL IisLOADALL286

Source & expected listing t3439.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=24, CPU=X64, UNDOC=ON | |t3439 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F05 | LOADALL286 |0002:0F07 | LOADALL |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F05 | LOADALL286 |00000002:0F07 | LOADALL |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F05 | LOADALL286 |00000002:0F07 | LOADALL | |ENDPROGRAM t3439`

Expected messages t3439.out
  `I0180 Assembling source file "t3439.htm". I0270 Assembling source "t3439". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3439". "t3439.htm"{52} I0510 Assembling program pass 1. "t3439.htm"{52} I0530 Assembling program pass 2 - final. "t3439.htm"{52} I0660 16bit TINY BIN file "t3439.bin" created, size=36. "t3439.htm"{62} I0650 Program "t3439" assembled in 2 passes with errorlevel 0. "t3439.htm"{62} I0750 Source "t3439" (80 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3439.htm.lst" created, size=623. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲