| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5270: Machine instructions VCOMPRESSPS VCOMPRESSPD VPCOMPRESSD VPCOMPRESSQ

Tested procedures
  IizVCOMPRESSPS IizVCOMPRESSPD IizVPCOMPRESSD IizVPCOMPRESSQ

Source & expected listing t5270.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=34, DUMPALL=OFF, CPU=X64, SIMD=AVX512, EVEX=ON | |t5270 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27D088AD1 | VCOMPRESSPS XMM1,XMM2 |00000006:62F27D8B8AD1 | VCOMPRESSPS XMM1,XMM2,MASK=K3,ZEROING=ON |0000000C:62F27D088A5510<2 | VCOMPRESSPS [RBP+40h],XMM2 |00000013:62F27D0B8A5510<2 | VCOMPRESSPS [RBP+40h],XMM2,MASK=K3 |0000001A:62F2FD088AD1 | VCOMPRESSPD XMM1,XMM2 |00000020:62F2FD8B8AD1 | VCOMPRESSPD XMM1,XMM2,MASK=K3,ZEROING=ON |00000026:62F2FD088A5508<3 | VCOMPRESSPD [RBP+40h],XMM2 |0000002D:62F2FD0B8A5508<3 | VCOMPRESSPD [RBP+40h],XMM2,MASK=K3 |00000034:62F27D088BD1 | VPCOMPRESSD XMM1,XMM2 |0000003A:62F27D8B8BD1 | VPCOMPRESSD XMM1,XMM2,MASK=K3,ZEROING=ON |00000040:62F27D088B5510<2 | VPCOMPRESSD [RBP+40h],XMM2 |00000047:62F27D0B8B5510<2 | VPCOMPRESSD [RBP+40h],XMM2,MASK=K3 |0000004E:62F2FD088BD1 | VPCOMPRESSQ XMM1,XMM2 |00000054:62F2FD8B8BD1 | VPCOMPRESSQ XMM1,XMM2,MASK=K3,ZEROING=ON |0000005A:62F2FD088B5508<3 | VPCOMPRESSQ [RBP+40h],XMM2 |00000061:62F2FD0B8B5508<3 | VPCOMPRESSQ [RBP+40h],XMM2,MASK=K3 | |ENDPROGRAM t5270`

Expected messages t5270.out
  `I0180 Assembling source file "t5270.htm". I0270 Assembling source "t5270". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5270". "t5270.htm"{58} I0510 Assembling program pass 1. "t5270.htm"{58} I0530 Assembling program pass 2 - final. "t5270.htm"{58} I0660 16bit TINY BIN file "t5270.bin" created, size=104. "t5270.htm"{76} I0650 Program "t5270" assembled in 2 passes with errorlevel 0. "t5270.htm"{76} I0750 Source "t5270" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5270.htm.lst" created, size=1419. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲