| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3336: Machine instructions BTC BTCW BTCD BTCQ

Tested procedures
  IigBTC IigBTCW IigBTCD IigBTCQ

Source & expected listing t3336.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,CPU=X64 | |t3336 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FBBD1 | BTC CX,DX |0003:660FBBD1 | BTC ECX,EDX |0007:0FBB14 | BTC [SI],DX |000A:660FBB14 | BTC [SI],EDX |000E:0FBB16[7C00] | BTC [MemWord],DX |0013:660FBB16[7800] | BTC [MemDword],EDX |0019:0FBAF902 | BTC CX,2 |001D:660FBAF902 | BTC ECX,2 |0022:0FBA3E[7C00]02 | BTC [MemWord],2 |0028:660FBA3E[7800]02 | BTC [MemDword],2 |002F:0FBA3C02 | BTCW [SI],2 |0033:660FBA3C02 | BTCD [SI],2 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660FBBD1 | BTC CX,DX |00000004:0FBBD1 | BTC ECX,EDX |00000007:660FBB16 | BTC [ESI],DX |0000000B:0FBB16 | BTC [ESI],EDX |0000000E:660FBB15[7C000000] | BTC [MemWord],DX |00000016:0FBB15[78000000] | BTC [MemDword],EDX |0000001D:660FBAF902 | BTC CX,2 |00000022:0FBAF902 | BTC ECX,2 |00000026:660FBA3D[7C000000]02 | BTC [MemWord],2 |0000002F:0FBA3D[78000000]02 | BTC [MemDword],2 |00000037:660FBA3E02 | BTCW [ESI],2 |0000003C:0FBA3E02 | BTCD [ESI],2 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:660FBBD1 | BTC CX,DX |00000004:0FBBD1 | BTC ECX,EDX |00000007:480FBBD1 | BTC RCX,RDX |0000000B:4D0FBBD1 | BTC R9,R10 |0000000F:660FBB16 | BTC [RSI],DX |00000013:0FBB16 | BTC [RSI],EDX |00000016:480FBB16 | BTC [RSI],RDX |0000001A:660FBB155A000000 | BTC [MemWord],DX |00000022:0FBB154F000000 | BTC [MemDword],EDX |00000029:480FBB153F000000 | BTC [MemQword],RDX |00000031:660FBAF902 | BTC CX,2 |00000036:0FBAF902 | BTC ECX,2 |0000003A:480FBAF902 | BTC RCX,2 |0000003F:490FBAF902 | BTC R9,2 |00000044:660FBA3D2F00000002 | BTC [MemWord],2 |0000004D:0FBA3D2300000002 | BTC [MemDword],2 |00000055:480FBA3D1200000002 | BTC [MemQword],2 |0000005E:660FBA3E02 | BTCW [RSI],2 |00000063:0FBA3E02 | BTCD [RSI],2 |00000067:480FBA3E02 | BTCQ [RSI],2 |0000006C:0F1F4000 | ALIGN QWORD |00000070:0000000000000000 |MemQword DQ Q |00000078:00000000 |MemDword DD D |0000007C:0000 |MemWord DW W | |ENDPROGRAM t3336`

Expected messages t3336.out
  `I0180 Assembling source file "t3336.htm". I0270 Assembling source "t3336". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3336". "t3336.htm"{58} I0510 Assembling program pass 1. "t3336.htm"{58} I0510 Assembling program pass 2. "t3336.htm"{58} I0510 Assembling program pass 3. "t3336.htm"{58} I0530 Assembling program pass 4 - final. "t3336.htm"{58} I0660 16bit TINY BIN file "t3336.bin" created, size=254. "t3336.htm"{110} I0650 Program "t3336" assembled in 4 passes with errorlevel 0. "t3336.htm"{110} I0750 Source "t3336" (130 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3336.htm.lst" created, size=2812. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲