| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4215: Machine instructions DMINT RDM BB0_RESET BB1_RESET CPU_WRITE CPU_READ

Description
  Deprecated AMD/Cyrix Geode instructions
Tested procedures
  IicDMINT IicRDM IicBB0_RESET IicBB1_RESET IicCPU_WRITE IicCPU_READ

Source & expected listing t4215.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=28, CPU=686, CYRIX=ON, UNDOC=ON | |t4215 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F39 | DMINT |0002:0F3A | RDM |0004:0F3A | BB0_RESET |0006:0F3B | BB1_RESET |0008:0F3C | CPU_WRITE |000A:0F3D | CPU_READ |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F39 | DMINT |00000002:0F3A | RDM |00000004:0F3A | BB0_RESET |00000006:0F3B | BB1_RESET |00000008:0F3C | CPU_WRITE |0000000A:0F3D | CPU_READ | |ENDPROGRAM t4215`

Expected messages t4215.out
  `I0180 Assembling source file "t4215.htm". I0270 Assembling source "t4215". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4215". "t4215.htm"{67} I0510 Assembling program pass 1. "t4215.htm"{67} I0530 Assembling program pass 2 - final. "t4215.htm"{67} I0660 16bit TINY BIN file "t4215.bin" created, size=28. "t4215.htm"{82} I0650 Program "t4215" assembled in 2 passes with errorlevel 0. "t4215.htm"{82} I0750 Source "t4215" (100 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4215.htm.lst" created, size=840. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲