| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5654: Machine instructions VSQRTSS VSQRTSD VSQRTPS VSQRTPD

Tested procedures
  IiyVSQRTSS IiyVSQRTSD IiyVSQRTPS IiyVSQRTPD

Source & expected listing t5654.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5654 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5EA51CB | VSQRTSS XMM1,XMM2,XMM3 |00000004:C4E16A51CB | VSQRTSS XMM1,XMM2,XMM3,PREFIX=VEX3 |00000009:62F16EDC51CB | VSQRTSS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON,ROUND=UP |0000000F:C5EA514D40 | VSQRTSS XMM1,XMM2,[RBP+40h] |00000014:C4E16A514D40 | VSQRTSS XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |0000001A:62F16E8C514D10<2 | VSQRTSS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000021:C5EB51CB | VSQRTSD XMM1,XMM2,XMM3 |00000025:C4E16B51CB | VSQRTSD XMM1,XMM2,XMM3,PREFIX=VEX3 |0000002A:62F1EFDC51CB | VSQRTSD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON,ROUND=UP |00000030:C5EB514D40 | VSQRTSD XMM1,XMM2,[RBP+40h] |00000035:C4E16B514D40 | VSQRTSD XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |0000003B:62F1EF8C514D08<3 | VSQRTSD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000042:C5F851CA | VSQRTPS XMM1,XMM2 |00000046:C5FC51CA | VSQRTPS YMM1,YMM2 |0000004A:C4E17851CA | VSQRTPS XMM1,XMM2,PREFIX=VEX3 |0000004F:C4E17C51CA | VSQRTPS YMM1,YMM2,PREFIX=VEX3 |00000054:62F17C8B51CA | VSQRTPS XMM1,XMM2,MASK=K3,ZEROING=ON |0000005A:62F17CAB51CA | VSQRTPS YMM1,YMM2,MASK=K3,ZEROING=ON |00000060:62F17C5B51CA | VSQRTPS ZMM1,ZMM2,MASK=K3,ROUND=UP |00000066:C5F8514D40 | VSQRTPS XMM1,[RBP+40h] |0000006B:C5FC514D40 | VSQRTPS YMM1,[RBP+40h] |00000070:C4E178514D40 | VSQRTPS XMM1,[RBP+40h],PREFIX=VEX3 |00000076:C4E17C514D40 | VSQRTPS YMM1,[RBP+40h],PREFIX=VEX3 |0000007C:62F17C8B514D04<4 | VSQRTPS XMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000083:62F17CAB514D02<5 | VSQRTPS YMM1,[RBP+40h],MASK=K3,ZEROING=ON |0000008A:62F17CCB514D01<6 | VSQRTPS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |00000091:62F17C9B514D10<2 | VSQRTPS XMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |00000098:62F17CBB514D10<2 | VSQRTPS YMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |0000009F:62F17CDB514D10<2 | VSQRTPS ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |000000A6:C5F951CA | VSQRTPD XMM1,XMM2 |000000AA:C5FD51CA | VSQRTPD YMM1,YMM2 |000000AE:C4E17951CA | VSQRTPD XMM1,XMM2,PREFIX=VEX3 |000000B3:C4E17D51CA | VSQRTPD YMM1,YMM2,PREFIX=VEX3 |000000B8:62F1FD8B51CA | VSQRTPD XMM1,XMM2,MASK=K3,ZEROING=ON |000000BE:62F1FDAB51CA | VSQRTPD YMM1,YMM2,MASK=K3,ZEROING=ON |000000C4:62F1FD5B51CA | VSQRTPD ZMM1,ZMM2,MASK=K3,ROUND=UP |000000CA:C5F9514D40 | VSQRTPD XMM1,[RBP+40h] |000000CF:C5FD514D40 | VSQRTPD YMM1,[RBP+40h] |000000D4:C4E179514D40 | VSQRTPD XMM1,[RBP+40h],PREFIX=VEX3 |000000DA:C4E17D514D40 | VSQRTPD YMM1,[RBP+40h],PREFIX=VEX3 |000000E0:62F1FD8B514D04<4 | VSQRTPD XMM1,[RBP+40h],MASK=K3,ZEROING=ON |000000E7:62F1FDAB514D02<5 | VSQRTPD YMM1,[RBP+40h],MASK=K3,ZEROING=ON |000000EE:62F1FDCB514D01<6 | VSQRTPD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON |000000F5:62F1FD9B514D08<3 | VSQRTPD XMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |000000FC:62F1FDBB514D08<3 | VSQRTPD YMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON |00000103:62F1FDDB514D08<3 | VSQRTPD ZMM1,[RBP+40h],MASK=K3,ZEROING=ON,BCST=ON | |ENDPROGRAM t5654`

Expected messages t5654.out
  `I0180 Assembling source file "t5654.htm". I0270 Assembling source "t5654". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5654". "t5654.htm"{58} I0510 Assembling program pass 1. "t5654.htm"{58} I0530 Assembling program pass 2 - final. "t5654.htm"{58} I0660 16bit TINY BIN file "t5654.bin" created, size=266. "t5654.htm"{106} I0650 Program "t5654" assembled in 2 passes with errorlevel 0. "t5654.htm"{106} I0750 Source "t5654" (124 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5654.htm.lst" created, size=3414. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲