| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4422: Machine instructions RORX SHLX SARX SHRX

Tested procedures
  IivRORX IivSHLX IivSARX IivSHRX

Source & expected listing t4422.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX2,ABM=ENABLED | |t4422 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:C4E37BF0CA03 | RORX ECX,EDX,3 |00000006:C4E37BF00E03 | RORX ECX,[ESI],3 |0000000C:C4E261F7CA | SHLX ECX,EDX,EBX |00000011:C4E261F70E | SHLX ECX,[ESI],EBX |00000016:C4E262F7CA | SARX ECX,EDX,EBX |0000001B:C4E262F70E | SARX ECX,[ESI],EBX |00000020:C4E263F7CA | SHRX ECX,EDX,EBX |00000025:C4E263F70E | SHRX ECX,[ESI],EBX |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E3FBF0CA03 | RORX RCX,RDX,3 |00000006:C4E3FBF00E03 | RORX RCX,[RSI],3 |0000000C:C4E2E1F7CA | SHLX RCX,RDX,RBX |00000011:C4E2E1F70E | SHLX RCX,[RSI],RBX |00000016:C4E2E2F7CA | SARX RCX,RDX,RBX |0000001B:C4E2E2F70E | SARX RCX,[RSI],RBX |00000020:C4E2E3F7CA | SHRX RCX,RDX,RBX |00000025:C4E2E3F70E | SHRX RCX,[RSI],RBX |0000002A:C4E37BF0CA03 | RORX ECX,EDX,3 |00000030:67C4E37BF00E03 | RORX ECX,[ESI],3 |00000037:C4E261F7CA | SHLX ECX,EDX,EBX |0000003C:67C4E261F70E | SHLX ECX,[ESI],EBX |00000042:C4E262F7CA | SARX ECX,EDX,EBX |00000047:67C4E262F70E | SARX ECX,[ESI],EBX |0000004D:C4E263F7CA | SHRX ECX,EDX,EBX |00000052:67C4E2E3F70E | SHRX RCX,[ESI],RBX |00000058:C462E3F74D40 | SHRX R9,[RBP+40h],RBX | |ENDPROGRAM t4422`

Expected messages t4422.out
  `I0180 Assembling source file "t4422.htm". I0270 Assembling source "t4422". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4422". "t4422.htm"{58} I0510 Assembling program pass 1. "t4422.htm"{58} I0530 Assembling program pass 2 - final. "t4422.htm"{58} I0660 16bit TINY BIN file "t4422.bin" created, size=142. "t4422.htm"{86} I0650 Program "t4422" assembled in 2 passes with errorlevel 0. "t4422.htm"{86} I0750 Source "t4422" (104 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4422.htm.lst" created, size=1615. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲