| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3208: Machine instructions IN, OUT

Tested procedures
  IigIN IigOUT

Source & expected listing t3208.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=38, CPU=X64, PRIV=ENABLE | |t3208 PROGRAM FORMAT=BIN,LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:EC | IN AL,DX |0001:ED | IN AX,DX |0002:66ED | IN EAX,DX |0004:E430 | IN AL,0x30 |0006:E530 | IN AX,0x30 |0008:66E530 | IN EAX,0x30 |000B:EE | OUT DX,AL |000C:EF | OUT DX,AX |000D:66EF | OUT DX,EAX |000F:E630 | OUT 0x30,AL |0011:E730 | OUT 0x30,AX |0013:66E730 | OUT 0x30,EAX |0016: | |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:EC | IN AL,DX |00000001:66ED | IN AX,DX |00000003:ED | IN EAX,DX |00000004:E430 | IN AL,0x30 |00000006:66E530 | IN AX,0x30 |00000009:E530 | IN EAX,0x30 |0000000B:EE | OUT DX,AL |0000000C:66EF | OUT DX,AX |0000000E:EF | OUT DX,EAX |0000000F:E630 | OUT 0x30,AL |00000011:66E730 | OUT 0x30,AX |00000014:E730 | OUT 0x30,EAX |00000016: | |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:EC | IN AL,DX |00000001:66ED | IN AX,DX |00000003:ED | IN EAX,DX |00000004:E430 | IN AL,0x30 |00000006:66E530 | IN AX,0x30 |00000009:E530 | IN EAX,0x30 |0000000B:EE | OUT DX,AL |0000000C:66EF | OUT DX,AX |0000000E:EF | OUT DX,EAX |0000000F:E630 | OUT 0x30,AL |00000011:66E730 | OUT 0x30,AX |00000014:E730 | OUT 0x30,EAX | | ENDPROGRAM t3208`

Expected messages t3208.out
  `I0180 Assembling source file "t3208.htm". I0270 Assembling source "t3208". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3208". "t3208.htm"{52} I0510 Assembling program pass 1. "t3208.htm"{52} I0530 Assembling program pass 2 - final. "t3208.htm"{52} I0660 16bit TINY BIN file "t3208.bin" created, size=86. "t3208.htm"{94} I0650 Program "t3208" assembled in 2 passes with errorlevel 0. "t3208.htm"{94} I0750 Source "t3208" (112 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3208.htm.lst" created, size=2395. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲