| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6110: Machine instructions VCVTFXPNTUDQ2PS VCVTFXPNTDQ2PS VCVTFXPNTPS2UDQ VCVTFXPNTPS2DQ VCVTFXPNTPD2UDQ VCVTFXPNTPD2DQ

Tested procedures
  IiyVCVTFXPNTUDQ2PS IiyVCVTFXPNTDQ2PS IiyVCVTFXPNTPS2UDQ IiyVCVTFXPNTPS2DQ IiyVCVTFXPNTPD2UDQ IiyVCVTFXPNTPD2DQ

Source & expected listing t6110.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6110 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F378CCCACA03 | VCVTFXPNTUDQ2PS ZMM1,ZMM2,3,MASK=K4,SAE=ON,EH=ON |00000007:62F3780CCA4D01<603 | VCVTFXPNTUDQ2PS ZMM1,[RBP+40h],3,MASK=K4,OPER=0 ; {16to16). |0000000F:62F3781CCA4D10<203 | VCVTFXPNTUDQ2PS ZMM1,[RBP+40h],3,MASK=K4,OPER=1 ; {1to16}. |00000017:62F378CCCBCA03 | VCVTFXPNTDQ2PS ZMM1,ZMM2,3,MASK=K4,SAE=ON,EH=ON |0000001E:62F3780CCB4D01<603 | VCVTFXPNTDQ2PS ZMM1,[RBP+40h],3,MASK=K4,OPER=0 ; {16to16). |00000026:62F3781CCB4D10<203 | VCVTFXPNTDQ2PS ZMM1,[RBP+40h],3,MASK=K4,OPER=1 ; {1to16}. |0000002E:62F379CCCACA03 | VCVTFXPNTPS2UDQ ZMM1,ZMM2,3,MASK=K4,SAE=ON,EH=ON |00000035:62F3790CCA4D01<603 | VCVTFXPNTPS2UDQ ZMM1,[RBP+40h],3,MASK=K4,OPER=0 ; {16to16). |0000003D:62F3791CCA4D10<203 | VCVTFXPNTPS2UDQ ZMM1,[RBP+40h],3,MASK=K4,OPER=1 ; {1to16}. |00000045:62F379CCCBCA03 | VCVTFXPNTPS2DQ ZMM1,ZMM2,3,MASK=K4,SAE=ON,EH=ON |0000004C:62F3790CCB4D01<603 | VCVTFXPNTPS2DQ ZMM1,[RBP+40h],3,MASK=K4,OPER=0 ; {16to16). |00000054:62F3791CCB4D10<203 | VCVTFXPNTPS2DQ ZMM1,[RBP+40h],3,MASK=K4,OPER=1 ; {1to16}. |0000005C:62F3FBCCCACA03 | VCVTFXPNTPD2UDQ ZMM1,ZMM2,3,MASK=K4,SAE=ON,EH=ON |00000063:62F3FB0CCA4D01<603 | VCVTFXPNTPD2UDQ ZMM1,[RBP+40h],3,MASK=K4,OPER=0 ; {8to8). |0000006B:62F3FB1CCA4D08<303 | VCVTFXPNTPD2UDQ ZMM1,[RBP+40h],3,MASK=K4,OPER=1 ; {1to8}. |00000073:62F3FBCCE6CA03 | VCVTFXPNTPD2DQ ZMM1,ZMM2,3,MASK=K4,SAE=ON,EH=ON |0000007A:62F3FB0CE64D01<603 | VCVTFXPNTPD2DQ ZMM1,[RBP+40h],3,MASK=K4,OPER=0 ; {8to8). |00000082:62F3FB1CE64D08<303 | VCVTFXPNTPD2DQ ZMM1,[RBP+40h],3,MASK=K4,OPER=1 ; {1to8}. | |ENDPROGRAM t6110`

Expected messages t6110.out
  `I0180 Assembling source file "t6110.htm". I0270 Assembling source "t6110". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6110". "t6110.htm"{64} I0510 Assembling program pass 1. "t6110.htm"{64} I0530 Assembling program pass 2 - final. "t6110.htm"{64} I0660 16bit TINY BIN file "t6110.bin" created, size=138. "t6110.htm"{84} I0650 Program "t6110" assembled in 2 passes with errorlevel 0. "t6110.htm"{84} I0750 Source "t6110" (102 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6110.htm.lst" created, size=1879. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲