| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5452: Machine instructions VSCATTERDPS VSCATTERDPD VSCATTERQPS VSCATTERQPD

Tested procedures
  IizVSCATTERDPS IizVSCATTERDPD IizVSCATTERQPS IizVSCATTERQPD

Source & expected listing t5452.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5452 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27D0BA3540D10<2 | VSCATTERQPS [XMM1+RBP+40h],XMM2,MASK=K3 |00000008:62F27D2BA3540D10<2 | VSCATTERQPS [YMM1+RBP+40h],XMM2,MASK=K3 |00000010:62F27D4BA3540D10<2 | VSCATTERQPS [ZMM1+RBP+40h],YMM2,MASK=K3 |00000018:62F2FD0BA3540D08<3 | VSCATTERQPD [XMM1+RBP+40h],XMM2,MASK=K3 |00000020:62F2FD2BA3540D08<3 | VSCATTERQPD [YMM1+RBP+40h],YMM2,MASK=K3 |00000028:62F2FD4BA3540D08<3 | VSCATTERQPD [ZMM1+RBP+40h],ZMM2,MASK=K3 |00000030:62F2FD0BA2540D08<3 | VSCATTERDPD [XMM1+RBP+40h],XMM2,MASK=K3 |00000038:62F2FD2BA2540D08<3 | VSCATTERDPD [XMM1+RBP+40h],YMM2,MASK=K3 |00000040:62F2FD4BA2540D08<3 | VSCATTERDPD [YMM1+RBP+40h],ZMM2,MASK=K3 |00000048:62F2F90BA2540D08<3 | VSCATTERDPD [ZMM1+RBP+40h],ZMM2,MASK=K3 ; MVEX only, no conversion. |00000050:62F27D0BA2540D10<2 | VSCATTERDPS [XMM1+RBP+40h],XMM2,MASK=K3 |00000058:62F27D2BA2540D10<2 | VSCATTERDPS [YMM1+RBP+40h],YMM2,MASK=K3 |00000060:62F27D4BA2540D10<2 | VSCATTERDPS [ZMM1+RBP+40h],ZMM2,MASK=K3 |00000068:62F2790BA2540D10<2 | VSCATTERDPS [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=0 ; No conversion. |00000070:62F2793BA2540D20<1 | VSCATTERDPS [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=3 ; {float16}. |00000078:62F2794BA2540D40 | VSCATTERDPS [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=4 ; {uint8}. |00000080:62F2795BA2540D40 | VSCATTERDPS [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=5 ; {sint8}. |00000088:62F2796BA2540D20<1 | VSCATTERDPS [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=6 ; {sint16}. |00000090:62F2797BA2540D20<1 | VSCATTERDPS [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=7 ; {uint16}. | |ENDPROGRAM t5452`

Expected messages t5452.out
  `I0180 Assembling source file "t5452.htm". I0270 Assembling source "t5452". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5452". "t5452.htm"{58} I0510 Assembling program pass 1. "t5452.htm"{58} I0530 Assembling program pass 2 - final. "t5452.htm"{58} I0660 16bit TINY BIN file "t5452.bin" created, size=152. "t5452.htm"{79} I0650 Program "t5452" assembled in 2 passes with errorlevel 0. "t5452.htm"{79} I0750 Source "t5452" (97 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5452.htm.lst" created, size=1894. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲