| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5634: Machine instructions VPSRAVW VPSRAVD VPSRAVQ

Tested procedures
  IizVPSRAVW IizVPSRAVD IizVPSRAVQ

Source & expected listing t5634.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5634 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F2ED0811CB | VPSRAVW XMM1,XMM2,XMM3 |00000006:62F2ED2C11CB | VPSRAVW YMM1,YMM2,YMM3,MASK=K4 |0000000C:62F2EDCC11CB | VPSRAVW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000012:62F2ED08114D04<4 | VPSRAVW XMM1,XMM2,[RBP+40h] |00000019:62F2ED2C114D02<5 | VPSRAVW YMM1,YMM2,[RBP+40h],MASK=K4 |00000020:62F2EDCC114D01<6 | VPSRAVW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000027:C4E26946CB | VPSRAVD XMM1,XMM2,XMM3 |0000002C:C4E26D46CB | VPSRAVD YMM1,YMM2,YMM3 |00000031:62F26D0C46CB | VPSRAVD XMM1,XMM2,XMM3,MASK=K4 |00000037:62F26D2C46CB | VPSRAVD YMM1,YMM2,YMM3,MASK=K4 |0000003D:62F26D4846CB | VPSRAVD ZMM1,ZMM2,ZMM3 |00000043:62F2692846CB | VPSRAVD ZMM1,ZMM2,ZMM3,EH=OFF,OPER=2 ; MVEX {badc}. |00000049:C4E269464D40 | VPSRAVD XMM1,XMM2,[RBP+40h] |0000004F:C4E26D464D40 | VPSRAVD YMM1,YMM2,[RBP+40h] |00000055:62F26D08464D04<4 | VPSRAVD XMM1,XMM2,[RBP+40h],BCST=OFF |0000005C:62F26D28464D02<5 | VPSRAVD YMM1,YMM2,[RBP+40h],BCST=OFF |00000063:62F26D48464D01<6 | VPSRAVD ZMM1,ZMM2,[RBP+40h],BCST=OFF |0000006A:62F26D18464D10<2 | VPSRAVD XMM1,XMM2,[RBP+40h],BCST=ON |00000071:62F26D38464D10<2 | VPSRAVD YMM1,YMM2,[RBP+40h],BCST=ON |00000078:62F26D58464D10<2 | VPSRAVD ZMM1,ZMM2,[RBP+40h],BCST=ON |0000007F:62F26908464D01<6 | VPSRAVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |00000086:62F26918464D10<2 | VPSRAVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |0000008D:62F26928464D04<4 | VPSRAVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |00000094:62F26948464D04<4 | VPSRAVD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |0000009B:62F2ED0846CB | VPSRAVQ XMM1,XMM2,XMM3 |000000A1:62F2ED2846CB | VPSRAVQ YMM1,YMM2,YMM3 |000000A7:62F2ED0C46CB | VPSRAVQ XMM1,XMM2,XMM3,MASK=K4 |000000AD:62F2ED2C46CB | VPSRAVQ YMM1,YMM2,YMM3,MASK=K4 |000000B3:62F2ED4846CB | VPSRAVQ ZMM1,ZMM2,ZMM3 |000000B9:62F2ED08464D04<4 | VPSRAVQ XMM1,XMM2,[RBP+40h] |000000C0:62F2ED28464D02<5 | VPSRAVQ YMM1,YMM2,[RBP+40h] |000000C7:62F2ED0C464D04<4 | VPSRAVQ XMM1,XMM2,[RBP+40h],MASK=K4 |000000CE:62F2ED2C464D02<5 | VPSRAVQ YMM1,YMM2,[RBP+40h],MASK=K4 |000000D5:62F2ED48464D01<6 | VPSRAVQ ZMM1,ZMM2,[RBP+40h] | |ENDPROGRAM t5634`

Expected messages t5634.out
  `I0180 Assembling source file "t5634.htm". I0270 Assembling source "t5634". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5634". "t5634.htm"{55} I0510 Assembling program pass 1. "t5634.htm"{55} I0530 Assembling program pass 2 - final. "t5634.htm"{55} I0660 16bit TINY BIN file "t5634.bin" created, size=220. "t5634.htm"{91} I0650 Program "t5634" assembled in 2 passes with errorlevel 0. "t5634.htm"{91} I0750 Source "t5634" (109 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5634.htm.lst" created, size=2581. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲