| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4144: Machine instructions HINT_NOP in 16bit mode

Tested procedures
  IisHINT_NOP

Source & expected listing t4144.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,UNDOC=ON | |t4144 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F18C2 | HINT_NOP 0,DX |0003:660F18C2 | HINT_NOP 0,EDX |0007:0F1804 | HINT_NOP 0,[SI],DATA=WORD |000A:0F1804 | HINT_NOPW 0,[SI] |000D:670F1806 | HINT_NOP 0,[ESI],DATA=WORD |0011:0F18C1 | HINT_NOP 00q,CX |0014:0F18C9 | HINT_NOP 01q,CX |0017:0F18D1 | HINT_NOP 02q,CX |001A:0F18D9 | HINT_NOP 03q,CX |001D:0F18E1 | HINT_NOP 04q,CX |0020:0F18E9 | HINT_NOP 05q,CX |0023:0F18F1 | HINT_NOP 06q,CX |0026:0F18F9 | HINT_NOP 07q,CX |0029:0F19C1 | HINT_NOP 10q,CX |002C:0F19C9 | HINT_NOP 11q,CX |002F:0F19D1 | HINT_NOP 12q,CX |0032:0F19D9 | HINT_NOP 13q,CX |0035:0F19E1 | HINT_NOP 14q,CX |0038:0F19E9 | HINT_NOP 15q,CX |003B:0F19F1 | HINT_NOP 16q,CX |003E:0F19F9 | HINT_NOP 17q,CX |0041:0F1AC1 | HINT_NOP 20q,CX |0044:0F1AC9 | HINT_NOP 21q,CX |0047:0F1AD1 | HINT_NOP 22q,CX |004A:0F1AD9 | HINT_NOP 23q,CX |004D:0F1AE1 | HINT_NOP 24q,CX |0050:0F1AE9 | HINT_NOP 25q,CX |0053:0F1AF1 | HINT_NOP 26q,CX |0056:0F1AF9 | HINT_NOP 27q,CX |0059:0F1BC1 | HINT_NOP 30q,CX |005C:0F1BC9 | HINT_NOP 31q,CX |005F:0F1BD1 | HINT_NOP 32q,CX |0062:0F1BD9 | HINT_NOP 33q,CX |0065:0F1BE1 | HINT_NOP 34q,CX |0068:0F1BE9 | HINT_NOP 35q,CX |006B:0F1BF1 | HINT_NOP 36q,CX |006E:0F1BF9 | HINT_NOP 37q,CX |0071:0F1CC1 | HINT_NOP 40q,CX |0074:0F1CC9 | HINT_NOP 41q,CX |0077:0F1CD1 | HINT_NOP 42q,CX |007A:0F1CD9 | HINT_NOP 43q,CX |007D:0F1FE1 | HINT_NOP 74q,CX |0080:0F1FE9 | HINT_NOP 75q,CX |0083:0F1FF1 | HINT_NOP 76q,CX |0086:0F1FF9 | HINT_NOP 77q,CX |0089:0F1FF9 | HINT_NOP 63,CX |008C:0F1F3C | HINT_NOPW 63,[SI] |008F:66670F1F3E | HINT_NOPD 63,[ESI] | |ENDPROGRAM t4144`

Expected messages t4144.out
  `I0180 Assembling source file "t4144.htm". I0270 Assembling source "t4144". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4144". "t4144.htm"{49} I0510 Assembling program pass 1. "t4144.htm"{49} I0530 Assembling program pass 2 - final. "t4144.htm"{49} I0660 16bit TINY BIN file "t4144.bin" created, size=148. "t4144.htm"{99} I0650 Program "t4144" assembled in 2 passes with errorlevel 0. "t4144.htm"{99} I0750 Source "t4144" (117 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4144.htm.lst" created, size=2662. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲